{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N7"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B7","3MXM52N2V1B7","3MXM68N2V1B7"]
["Ventilator","Luftstromvolumen","Kühlen","Sehr niedrig","m³/min","","","24.1"]
["","","Heizen","Sehr niedrig","m³/min","","","24.1"]
["","","","Sehr niedrig","cfm","","","851"]
["","","Heizen","Sehr niedrig","cfm","","","851"]
["Abmessungen","Maßeinheit","","Höhe","mm","734","734","734"]
["","","","Breite","mm","974","974","958"]
["","","","Tiefe","mm","401","401","340"]
["Gewicht","Maßeinheit","","","kg","57","57","62"]
["Ventilatormotor","Drehzahl","Kühlen","Sehr niedrig","U/min","420","420"]
["","","Heizen","Sehr niedrig","U/min","420","420"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°CTK","-10","-10","-10"]
["","","","Max.","°CTK","46","46","46"]
["Schalldruckpegel","Kühlen","","Nom.","dBA","46","46","48"]
["","Heizen","","Nom.","dBA","47","47","48"]
["Kältemittel","Typ","","","","R-32","R-32","R-32"]
["","Füllmenge","","","kg","1.8","1.8","2"]
["","Füllmenge","","","tCO2Eq","1.22","1.22"]
["","GWP","","","","675","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","Außengerät – Innengerät","m","25","25 (1)","25"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 30 m)","0,02 (für Rohrleitungslängen über 30 m)","0,02 (für Rohrleitungslängen über 30 m)"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","15.0","15.0","15"]
["","","Innengerät – Innengerät","Max.","m","7.5","7.5","7.5"]
["","Gesamtleitungslänge","System","Ist","m","50","50 (2)","50"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["","Reducer assembly","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["","Spannung","","","V","220-240","220-240","220-440"]
["Hinweise","","","","","(1) - Für 1 Raum","(1) - Für 1 Raum"]
["","","","","","(2) - Bei Kombination mit CVXM-A, FVXM-A – maximale Rohrleitungslänge 30 m.","(2) - Bei Kombination mit CVXM-A, FVXM-A – maximale Rohrleitungslänge 30 m."]
["Verdichter","Typ","","","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Heizen","Umgebung","Betriebsbereich-=-Heizen-=-Umgebung-=-Min.-=-°C FK","°C FK","","","-15"]
["","","","Betriebsbereich-=-Heizen-=-Umgebung-=-Max.-=-°C FK","°C FK","","","24"]
["Energieeffizienzbereich","","","","","","","A+++ ~ D"]