{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":7,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-A9"]
[]
[]
[]
[]
["","","","","","4MXM68A2V1B9","4MXM80A2V1B9"]
["Abmessungen","Maßeinheit","","Höhe","mm","734","734"]
["","","","Breite","mm","974","974"]
["","","","Tiefe","mm","408","408"]
["Gewicht","Maßeinheit","","","kg","63","67"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°C TK","-10","-10"]
["","","","Max.","°C TK","46","46"]
["Schalldruckpegel","Kühlen","","Nom.","dBA","48","48"]
["","Heizen","","Nom.","dBA","49","49"]
["Kältemittel","Typ","","","","R-32","R-32"]
["","Füllmenge","","","kg","2","2.4"]
["","Füllmenge","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","Außengerät – Innengerät","m","25 (1)","25 (1)"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 30 m)","0,02 (für Rohrleitungslängen über 30 m)"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","15","15"]
["","","Innengerät – Innengerät","Max.","m","7.5","7.5"]
["","Gesamtleitungslänge","System","Ist","m","60","70"]
["Standardzubehör","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Stromversorgung","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["","Spannung","","","V","220-240","220-240"]
["Hinweise","","","","","(1) - Für 1 Raum","(1) - Für 1 Raum"]