{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-N"]
[]
[]
[]
[]
["","","","","","4MXM68N2V1B (Archived)","4MXM80N2V1B (Archived)"]
["Ventilator","Luftstromvolumen","Kühlen","Sehr niedrig","m³/min","24.1","24.1"]
["","","Heizen","Sehr niedrig","m³/min","24.1","24.1"]
["","","","Sehr niedrig","cfm","851","851.0"]
["","","Heizen","Sehr niedrig","cfm","851.0","851.0"]
["Abmessungen","Maßeinheit","","Höhe","mm","734","734"]
["","","","Breite","mm","958","958"]
["","","","Tiefe","mm","340","340"]
["Gewicht","Maßeinheit","","","kg","63","67"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°CTK","-10","-10"]
["","","","Max.","°CTK","46","46"]
["","Heizen","Umgebung","Min.","°C FK","-15","-15"]
["","","","Max.","°C FK","18","18"]
["Schalldruckpegel","Kühlen","","Nom.","dBA","48","49"]
["","Heizen","","Nom.","dBA","48","49"]
["Kältemittel","Typ","","","","R-32","R-32"]
["","Füllmenge","","","kg","2.00","2.40"]
["","Füllmenge","","","tCO2Eq","1.4","1.6"]
["","GWP","","","","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","Außengerät – Innengerät","m","25","25"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 30 m)","0,02 (für Rohrleitungslängen über 30 m)"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","15","15"]
["","","Innengerät – Innengerät","Max.","m","7.5","7.5"]
["","Gesamtleitungslänge","System","Ist","m","60","70"]
["Standardzubehör","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Stromversorgung","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["","Spannung","","","V","220-240","220-240"]