{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-N9"]
[]
[]
[]
[]
["","","","","","5MXM90N2V1B9"]
["Abmessungen","Maßeinheit","","Höhe","mm","734"]
["","","","Breite","mm","974"]
["","","","Tiefe","mm","401"]
["Gewicht","Maßeinheit","","","kg","68"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°C Trockenkugel","-10"]
["","","","Max.","°C Trockenkugel","46"]
["Schalldruckpegel","Kühlen","","Nom.","dBA","52"]
["","Heizen","","Nom.","dBA","52.0"]
["Kältemittel","Typ","","","","R-32"]
["","Füllmenge","","","kg","2.4"]
["","Füllmenge","","","tCO2Eq","1.62"]
["","GWP","","","","675.0"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","Außengerät – Innengerät","m","25 (1)"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 30 m)"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","15.0"]
["","","Innengerät – Innengerät","Max.","m","7.5"]
["","Gesamtleitungslänge","System","Ist","m","75"]
["Stromversorgung","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["","Spannung","","","V","220-240"]
["Standardzubehör","Installation manual","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Hinweise","","","","","(1) - Für 1 Raum"]