{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5XXM-A"]
[]
[]
[]
[]
["","","","","","5XXM68A2V1B","5XXM90A2V1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","734","734"]
["","","","Breite","mm","1040","1040"]
["","","","Tiefe","mm","408","408"]
["Gewicht","Maßeinheit","","","kg","69.0","73.0"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°C TK","-10","-10"]
["","","","Max.","°C TK","50","50"]
["Schalldruckpegel","Kühlen","","Nom.","dB(A)","48.0 (2)","52.0 (2)"]
["","Heizen","","Nom.","dB(A)","49.0 (2), 51.0 (3)","53.0 (2), 55.0 (3)"]
["Kältemittel","Typ","","","","R-32","R-32"]
["","Füllmenge","","","kg","2.00","2.40"]
["","Kältemittel-=-Füllmenge-=-tCO2-Äq.","","","tCO2-Äq.","1.35","1.62"]
["","GWP","","","","675","675.0"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","Außengerät – Innengerät","m","25 (4) (5)","25 (5) (4)"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 30 m)","0,02 (für Rohrleitungslängen über 30 m)"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","15.0 (5)","15.0 (5)"]
["","","Innengerät – Innengerät","Max.","m","7.5 (5)","7.5 (5)"]
["","Gesamtleitungslänge","System","Ist","m","60","75"]
["Standardzubehör","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","2","2"]
["Energieeffizienzbereich","","","","","A+++ ~ D","A+++ ~ D"]
["Stromversorgung","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["","Spannung","","","V","220-240","220-240"]
["Hinweise","","","","","(1) - Angaben zu Betriebsbereichen: siehe gesonderte Zeichnung.","(1) - Angaben zu Betriebsbereichen: siehe gesonderte Zeichnung."]
["","","","","","(2) - For DX combination","(2) - For DX combination"]
["","","","","","(3) - For Space heating operation of CHVX07 unit","(3) - For Space heating operation of CHVX07 unit"]
["","","","","","(4) - Für 1Raum","(4) - Für 1Raum"]
["","","","","","(5) - For combination with FBA71/100/125 refer to installation manual","(5) - For combination with FBA71/100/125 refer to installation manual"]
["","","","","","(6) - Enthält fluorierte Treibhausgase","(6) - Enthält fluorierte Treibhausgase"]