{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / AZAS-MV"]
[]
[]
[]
[]
["","","","","ADEA100A2VEB / AZAS100MUV","ADEA125A2VEB / AZAS125MUV"]
["Kühlleistung","Nom.","","kW","9.5","12.1 (1)"]
["Heizleistung","Nom.","","kW","10.8 (2)","13.5 (2)"]
["Raumkühlen","Energieeffizienzklasse","","","A"]
["","Leistung","Pdesign","kW","9.5","12.1"]
["","SEER","","","5.55","5.11"]
["","Jährlicher Energieverbrauch","","kWh/a","600","1421"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A"]
["","Leistung","Pdesign","kW","6","6"]
["","SCOP/A","","","3.81","3.5"]
["","Jährlicher Energieverbrauch","","kWh/a","2205","2400"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]