{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ADEA100A2VEB / AZQS100B8V1B","ADEA125A2VEB / AZQS125B8V1B"]
["Kühlleistung","Nom.","","kW","9.50","12.10"]
["Raumkühlen","SEER","","","5.10","4.83"]
["","Jährlicher Energieverbrauch","","kWh/a","652","1,504"]
["","Leistung","Pdesign","kW","9.50","12.10"]
["","Energieeffizienzklasse","","","A"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","7.60","7.93"]
["","SCOP/A","","","3.81","3.50"]
["","Energieeffizienzklasse","","","A"]
["","Jährlicher Energieverbrauch","","kWh/a","2,793","3,167"]
["Nominale Effizienz","EER","","","","2.27"]
["Heizleistung","Nom.","","kW","10.80","13.50"]
["Hinweise","","","","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","(3) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m; Niveauunterschied: 0 m","(3) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m; Niveauunterschied: 0 m"]
["","","","","(4) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 7,5 m; Niveauunterschied: 0 m","(4) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 7,5 m; Niveauunterschied: 0 m"]