{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":11,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXC-B"]
[]
[]
[]
[]
["","","","","","ARXC20BV1B","ARXC25BV1B","ARXC35BV1B","ARXC50BV1B","ARXC60BV1B","ARXC71BV1B"]
["Schalldruckpegel","Kühlen","","Hoch","dBA","45","","","51","54"]
["Kältemittel","Charge","","","TCO2-Äquivalent","0.371","","","0.675","0.743"]
["","GWP","","","","675","","","675","675"]
["","Füllmenge","","","kg","0.55","","","1","1.1"]
["","Typ","","","","R-32","","","R-32","R-32"]
["Rohrleitungsanschlüsse","Niveauunterschied","Innengerät – Außengerät","Max.","m","15","","","20","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,017 (für Rohrleitungslängen über 7,5 m)","","","0,017 (für Rohrleitungslängen über 7,5 m)","0,017 (für Rohrleitungslängen über 7,5 m)"]
["Verdichter","Typ","","","","Hermetischer Swing","","","Hermetischer Swing","Hermetischer Swing"]
["Abmessungen","Maßeinheit","","Breite","mm","658","","","845","845"]
["","","","Tiefe","mm","273","","","300","300"]
["","","","Höhe","mm","550","","","615","615"]
["Gewicht","Maßeinheit","","","kg","24","","","39","39"]
["Power supply","Phase","","","","1~","","","1~","1~"]
["","Frequenz","","","Hz","50","","","50","50"]
["","Spannung","","","V","220-240","","","220-240","220-240"]
["Abmessungen","Maßeinheit","","Höhe","mm","","550","550","","","695"]
["","","","Breite","mm","","658","658","","","930"]
["","","","Tiefe","mm","","273","273","","","350"]
["Gewicht","Maßeinheit","","","kg","","24","26","","","45"]
["Verdichter","Typ","","","","","Hermetischer Swing","Hermetischer Swing","","","Hermetischer Swing"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°CTK","","10","10","","","-10"]
["","","","Max.","°CTK","","46","46","","","46"]
["","Heizen","Umgebung","Min.","°C FK","","-15","-15","","","-15"]
["","","","Max.","°C FK","","18","18","","","18"]
["Schalldruckpegel","Kühlen","","Hoch","dBA","","45","46","","","54"]
["Kältemittel","Typ","","","","","R-32","R-32","","","R-32"]
["","Füllmenge","","","kg","","0.55","0.75","","","1.15"]
["","Füllmenge","","","tCO2Eq","","0.371","0.506","","","0.776"]
["","GWP","","","","","675","675","","","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","Außengerät – Innengerät","m","","20","20","","","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","0,017 (für Rohrleitungslängen über 7,5 m)","0,017 (für Rohrleitungslängen über 7,5 m)","","","0,017 (für Rohrleitungslängen über 7,5 m)"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","","15","15","","","20"]
["Stromversorgung","Phase","","","","","1~","1~","","","1~"]
["","Frequenz","","","Hz","","50","50","","","50"]
["","Spannung","","","V","","220-240","220-240","","","220-240"]