{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-A"]
[]
[]
[]
[]
["","","","","","ARXM25A5V1B","ARXM35A5V1B","ARXM50A5V1B","ARXM60A5V1B","ARXM71A5V1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","610","610","734","734","734"]
["","","","Breite","mm","923","923","954","954","954"]
["","","","Tiefe","mm","367","367","401","401","401"]
["Gewicht","Maßeinheit","","","kg","36","36","49","49","49"]
["Ventilatormotor","Drehzahl","Kühlen","Sehr niedrig","U/min","600","600","500"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°C TK","-10","-10","-10","-10","-10"]
["","","","Max.","°C TK","50","50","50 (1), 46 (1)","46","46"]
["","Heizen","Umgebung","Betriebsbereich-=-Heizen-=-Umgebung-=-Min.-=-°C FK","°C FK","-21","-21","-21 (1), -15 (1)","-15","-15"]
["","","","Betriebsbereich-=-Heizen-=-Umgebung-=-Max.-=-°C FK","°C FK","18","18","18","18","18"]
["Schalldruckpegel","Kühlen","","Nom.","dB(A)","46","47","48","48","52"]
["","Heizen","","Nom.","dB(A)","47","49","49","49","52"]
["Kältemittel","Typ","","","","R-32","R-32","R-32","R-32","R-32"]
["","Füllmenge","","","kg","0.95","0.95","1.1","1.15","1.15"]
["","Kältemittel-=-Füllmenge-=-tCO2-Äq.","","","tCO2-Äq.","0.65","0.65","0.75","0.78","0.78"]
["","GWP","","","","675","675","675","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","Außengerät – Innengerät","m","20","20","30","30","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","002 (für Rohrleitungslängen über 10 m)","002 (für Rohrleitungslängen über 10 m)","002 (für Rohrleitungslängen über 10 m)","002 (für Rohrleitungslängen über 10 m)","0035 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","15","15","20","20","20"]
["Standardzubehör","Installation manual","","","","1","1","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","1","3","3"]
["Energieeffizienzbereich","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50","50"]
["","Spannung","","","V","220-240","220-240","220-240","220-240","220-240"]
["Hinweise","","","","","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase"]
["Standardzubehör","ARXM50A5V1B","","","","","","1"]
["","Drain plug","","","","","","","1","1"]