{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXC-B / ARXC-B"]
[]
[]
[]
[]
["","","","","ATXC20BV1B / ARXC20BV1B","ATXC25BV1B / ARXC25BV1B","ATXC35BV1B / ARXC35BV1B","ATXC50BV1B / ARXC50BV1B","ATXC60BV1B / ARXC60BV1B","ATXC71BV1B / ARXC71BV1B"]
["Außengerät","","","","ARXC20BV1B","ARXC25BV1B","ARXC35BV1B","ARXC50BV1B","ARXC60BV1B","RXC71BV1B"]
["Kühlleistung","Min.","","kW","1.30","1.30","1.30","1.37","1.80","2.30"]
["","Max.","","kW","3.00","3.00","4.00","6.20","7.00","7.30"]
["Heizleistung","Min.","","kW","1.30","1.30","1.30","1.36","1.48","2.30"]
["","Max.","","kW","4.00","4.00","4.80","6.60","8.00","9.00"]
["Nominale Effizienz","EER","","","3.33","3.30","3.30","3.25","3.25","2.95"]
["","COP","","","3.73","3.76","3.72","3.71","3.71","3.21"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A","A","A","A","C"]
["","","Heizen","","A","A","A","A","A","C"]
["Raumkühlen","Energieeffizienzklasse","","","A++","A++","A++","A++","A++","A"]
["","Leistung","Pdesign","kW","2.08","2.57","3.44","5.08","6.21","6.96"]
["","SEER","","","6.81","6.74","6.78","6.40","6.38","5.25"]
["","Jährlicher Energieverbrauch","","kWh/a","107","133","178","278","341","464"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A+","A+","A+","A+","A+","A"]
["","Leistung","Pdesign","kW","1.87","2.23","2.24","3.90","4.10","6.35"]
["","SCOP/A","","","4.39","4.41","4.26","4.37","4.19","3.81"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","1.38","1.57","1.71","2.99","3.49","5.36"]
["","Jährlicher Energieverbrauch","","kWh/a","595","707","736","1250","1373","2334"]
["Energieeffizienzbereich","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]