{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":11,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EAVX-D6V / EPGA011-016DV"]
[]
[]
[]
[]
["","","","","","EAVX16S18DA6V / EPGA11DAV3","EAVX16S23DA6V / EPGA11DAV3","EAVX16S18DA6V / EPGA14DAV3","EAVX16S23DA6V / EPGA14DAV3","EAVX16S18DA6V / EPGA16DAV3","EAVX16S23DA6V / EPGA16DAV3"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","L","","L","XL","L","XL"]
["","Durchschnittliches Klima","","Energieeffizienzklasse Wasserheizung","","A","","A","A","A","A"]
["COP","","","","","5.15 (1), 3.88 (2)","5.15, 3.88","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)"]
["Innengerät","","","","","EAVX16S18DA6V","EAVX16S23DA6V","EAVX16S18DA6V","EAVX16S23DA6V","EAVX16S18DA6V","EAVX16S23DA6V"]
["Kühlleistung","Nom.","","","kW","10.5 (1), 10.7 (2)","","11.1 (1), 11.9 (2)","11.1 (1), 11.9 (2)","13.5 (1), 11.9 (2)","13.5 (1), 11.9 (2)"]
["EER","","","","","4.75 (1), 3.23 (2)","4.75, 3.23","4.09 (1), 2.99 (2)","4.09 (1), 2.99 (2)","3.94 (1), 2.99 (2)","3.94 (1), 2.99 (2)"]
["Heizleistung","Nom.","","","kW","11.1 (1), 11.3 (2)","","14.5 (1), 14.5 (2)","14.5 (1), 14.5 (2)","16.5 (1), 15.6 (2)","16.5 (1), 15.6 (2)"]
["Leistungsaufnahme","Kühlen","","Nom.","kW","2.21 (1), 3.30 (2)","","2.72 (1), 3.97 (2)","2.72 (1), 3.97 (2)","3.42 (1), 3.97 (2)","3.42 (1), 3.97 (2)"]
["","Heizen","","Nom.","kW","2.16 (1), 2.91 (2)","","2.91 (1), 3.96 (2)","2.91 (1), 3.96 (2)","3.45 (1), 4.21 (2)","3.45 (1), 4.21 (2)"]
["Hinweise","","","","","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7℃ (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7℃ (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7℃ (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7℃ (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7℃ (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7℃ (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45℃ (DT = 5°C)"]
["Heizleistung","Nom.","","","kW","","11.1, 11.3"]
["Kühlleistung","Nom.","","","kW","","10.5, 10.7"]
["Leistungsaufnahme","Heizen","","Nom.","kW","","2.16, 2.91"]
["","Kühlen","","Nom.","kW","","2.21, 3.30"]
["","Leistungsaufnahme-=-Warmwasser von 10&nbsp;°C bis 50&nbsp;°C","","Leistungsaufnahme-=-Warmwasser von 10&nbsp;°C bis 50&nbsp;°C-=-Nom.-=-kWh","kWh","","3.08"]
["Aufwärmzeit von 10&nbsp;°C bis 50&nbsp;°C-=-h","h","","","","","9 h 20 min bei 7 °C Umgebungstemperatur"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","","XL"]
["","Durchschnittliches Klima","","Energieeffizienzklasse Wasserheizung","","","A"]
["Raumheizen","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein-=-SCOP","","","3.32"]
["","","","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein-=-Saisonale Effizienzklasse Raumheizen","","","A++"]
["","Wasserauslass 35°C für durchschnittliches Klima","Allgemein","SCOP","","","4.44"]
["","","","Saisonale Effizienzklasse Raumheizen","","","A+++"]