{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E6V / ERGA-EVH"]
[]
[]
[]
[]
["","","","","","EHVX08S18EA6V / ERGA06EAV3H","EHVX08S18EJ6V / ERGA06EAV3H","EHVX08S23EA6V / ERGA06EAV3H","EHVX08S23EJ6V / ERGA06EAV3H"]
["Heizleistung","Nom.","","","kW","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)"]
["Kühlleistung","Nom.","","","kW","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)"]
["Leistungsaufnahme","Heizen","","Nom.","kW","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)"]
["","Kühlen","","Nom.","kW","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)"]
["","Leistungsaufnahme-=-Warmwasser von 10 °C bis 50 °C","","Leistungsaufnahme-=-Warmwasser von 10 °C bis 50 °C-=-Nom.-=-kWh","kWh","2.48","2.48","3.01","3.01"]
["Aufwärmzeit von 10°C bis 50°C","h","","","","1h 28min","1h 28min","1h 40min","1h 40min"]
["COP","","","","","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)"]
["EER","","","","","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","L","L","XL","XL"]
["","Durchschnittliches Klima","","Energieeffizienzklasse Wasserheizung","","A+","A+","A+","A+"]
["Raumheizen","Raumheizen-=-Wasserauslass 55 °C für durchschnittliches Klima","Raumheizen-=-Wasserauslass 55 °C für durchschnittliches Klima-=-Allgemein","Raumheizen-=-Wasserauslass 55 °C für durchschnittliches Klima-=-Allgemein-=-SCOP","","3.28","3.27","3.28","3.28"]
["","","","Raumheizen-=-Wasserauslass 55 °C für durchschnittliches Klima-=-Allgemein-=-Saisonale Effizienzklasse Raumheizen","","A++","A++","A++","A++"]
["","Wasserauslass 35°C für durchschnittliches Klima","Allgemein","SCOP","","4.52","4.52","4.52","4.52"]
["","","","Saisonale Effizienzklasse Raumheizen","","A+++","A+++","A+++","A+++"]
["Energieeffizienzbereich","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Hinweise","","","","","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45°C (DT = 5°C)"]