{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":5,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKRTW"]
[]
[]
[]
[]
["","","","","EKRTWA"]
["Regelungsfunktion","","","","Proportionales Band"]
["Abmessungen","Maßeinheit","Breite","mm","125"]
["","","Tiefe","mm","34"]
["","","Höhe","mm","87"]
["Bereich der Temperatureinstellung","Heizen","Max.","°C","37"]
["","","Min.","°C","4"]
["","Kühlen","Max.","°C","37"]
["","","Min.","°C","4"]
["Uhr","","","","Ja"]
["Gewicht","Gerät","","g","215"]
["Umgebungstemperatur","Lagerung","Min.","°C","-20"]
["","","Max.","°F","140"]
["","","Min.","°F","-4"]
["","","Max.","°C","60"]
["","Betrieb","Min.","°C","0"]
["","","Max.","°F","122"]
["","","Min.","°F","32"]
["","","Max.","°C","50"]
["Maximaler Nenn-Schaltstrom (bei 230V~)","A","","","5.0 (1)"]
["Anschluss","Typ","","","Mit Kabel"]
["Power supply","Spannung","","V","Batteriebetrieben 3* AA-LR6 (Alkali)"]
["Hinweise","","","","(1) - 230 V~"]