{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":8,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELBH-E6V / ERRA08-12EV3"]
[]
[]
[]
[]
["","","","","","ELBH12EF6V / ERRA08EAV3","ELBH12EF6V / ERRA10EAV3","ELBH12EF6V / ERRA12EAV3"]
["Heizleistung","Min.","","","kW","3.45","3.45","3.45"]
["","Nom.","","","kW","6.17","6.17","6.17"]
["","Max.","","","kW","7.95","9.25","9.97"]
["Leistungsaufnahme","Heizen","","Min.","kW","0.72","0.72","0.72"]
["","","","Nom.","kW","1.25","1.25","1.25"]
["","","","Max.","kW","1.69","2.04","2.28"]
["COP","","","","","4.92","4.92","4.92"]
["Raumheizen","Raumheizen-=-Wasserauslass 55 °C für durchschnittliches Klima","Raumheizen-=-Wasserauslass 55 °C für durchschnittliches Klima-=-Allgemein","Raumheizen-=-Wasserauslass 55 °C für durchschnittliches Klima-=-Allgemein-=-SCOP","","3.34","3.34","3.44"]
["","","","Raumheizen-=-Wasserauslass 55 °C für durchschnittliches Klima-=-Allgemein-=-Saisonale Effizienzklasse Raumheizen","","A++","A++","A++"]
["","Wasserauslass 35°C für durchschnittliches Klima","Allgemein","SCOP","","4.69","4.71","4.71"]
["","","","Saisonale Effizienzklasse Raumheizen","","A+++","A+++","A+++"]
["Hinweise","","","","","(1) - Leistung entsprechend Norm EN 14511 und gültig für geheiztes Wasser im Bereich dT = 3 bis 8 °C bei Ta 7 °C","(1) - Leistung entsprechend Norm EN 14511 und gültig für geheiztes Wasser im Bereich dT = 3 bis 8 °C bei Ta 7 °C","(1) - Leistung entsprechend Norm EN 14511 und gültig für geheiztes Wasser im Bereich dT = 3 bis 8 °C bei Ta 7 °C"]
["","","","","","(2) - Bedingung: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Bedingung: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Bedingung: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Die Leistungsaufnahme ergibt sich aus der Gesamt-Leistungsaufnahme von Innengeräten und Außengeräten, einschließlich Umwälzpumpe; entsprechend EN14511","(3) - Die Leistungsaufnahme ergibt sich aus der Gesamt-Leistungsaufnahme von Innengeräten und Außengeräten, einschließlich Umwälzpumpe; entsprechend EN14511","(3) - Die Leistungsaufnahme ergibt sich aus der Gesamt-Leistungsaufnahme von Innengeräten und Außengeräten, einschließlich Umwälzpumpe; entsprechend EN14511"]
["","","","","","(4) - 7°C/6°CTK/FK - LWC35°C (dT=5°C) bei Pumpe auf voller Drehzahl","(4) - 7°C/6°CTK/FK - LWC35°C (dT=5°C) bei Pumpe auf voller Drehzahl","(4) - 7°C/6°CTK/FK - LWC35°C (dT=5°C) bei Pumpe auf voller Drehzahl"]