{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELSXB-E"]
[]
[]
[]
[]
["","","","","","ELSXB12P30EF","ELSXB12P50EF","ELSXB12P30EG","ELSXB12P50EG"]
["Gehäuse","Farbe","","","","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)"]
["","Material","","","","Schlagfestes Polypropylen","Schlagfestes Polypropylen","Schlagfestes Polypropylen","Schlagfestes Polypropylen"]
["Abmessungen","Maßeinheit","","Höhe","mm","1,893","1,910","1891","1910"]
["","","","Breite","mm","594","792","594","792"]
["","","","Tiefe","mm","680","817","680","817"]
["Gewicht","Maßeinheit","","","kg","76.0","91.0","93.0","115"]
["PED","Kategorie","","","","Kategorie II","Kategorie II","Kategorie II","Kategorie II"]
["Kältemittel","Typ","","","","R-32","R-32","R-32","R-32"]
["Schallleistungspegel","Schallleistungspegel-=-Nom.-=-dB(A)","","","dB(A)","44.7","44.7","44.7","44.7"]
["Schalldruckpegel","Nom.","","","dB(A)","36.8","36.8","36.8","36.8"]
["Betriebsbereich","Heizen","Wasserseite","Min.","°C","15 (3)","15 (3)","15 (3)","15 (3)"]
["","","","Max.","°C","65 (3)","65 (3)","65 (3)","65 (3)"]
["","Kühlen","Umgebung","Min.","°C TK","10 (3)","10 (3)","10 (3)","10 (3)"]
["","","Wasserseite","Min.","°C","5 (3)","5 (3)","5 (3)","5 (3)"]
["","","","Max.","°C","22 (3)","22 (3)","22 (3)","22 (3)"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50"]
["","Spannung","","","V","230","230","230","230"]
["Hinweise","","","","","(1) - Betriebsbereich wird je nach Betriebsart auf niedrigere Durchflussraten erweitert-siehe ESP-Kurve.","(1) - Betriebsbereich wird je nach Betriebsart auf niedrigere Durchflussraten erweitert-siehe ESP-Kurve.","(1) - Betriebsbereich wird je nach Betriebsart auf niedrigere Durchflussraten erweitert-siehe ESP-Kurve.","(1) - Betriebsbereich wird je nach Betriebsart auf niedrigere Durchflussraten erweitert-siehe ESP-Kurve."]
["","","","","","(2) - Wärmeverlust gemäß EN12897","(2) - Wärmeverlust gemäß EN12897","(2) - Wärmeverlust gemäß EN12897","(2) - Wärmeverlust gemäß EN12897"]
["","","","","","(3) - Weitere Informationen in der Betriebsbereichszeichnung.","(3) - Weitere Informationen in der Betriebsbereichszeichnung.","(3) - Weitere Informationen in der Betriebsbereichszeichnung.","(3) - Weitere Informationen in der Betriebsbereichszeichnung."]