{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EV"]
[]
[]
[]
[]
["","","","","","ERGA04EAV3"]
["Abmessungen","Maßeinheit","","Höhe","mm","740"]
["","","","Breite","mm","884"]
["","","","Tiefe","mm","388"]
["Gewicht","Maßeinheit","","","kg","58.5"]
["Betriebsbereich","Kühlung","","Betriebsbereich-=-Kühlung-=-Min.-=-°C&nbsp;TK","°C TK","10"]
["","","","Betriebsbereich-=-Kühlung-=-Max.-=-°C&nbsp;TK","°C TK","43"]
["","Warmwasser","","Min.","°C TK","-25"]
["","","","Betriebsbereich-=-Warmwasser-=-Max.-=-°C&nbsp;TK","°C TK","35"]
["Schallleistungspegel","Heizen","","Nom.","dB(A)","58 (1)"]
["","Kühlen","","Nom.","dB(A)","61 (1)"]
["Schalldruckpegel","Heizen","","Nom.","dB(A)","44 (1)"]
["","Kühlen","","Nom.","dB(A)","48 (1)"]
["Kältemittel","Typ","","","","R-32"]
["","GWP","","","","675.0"]
["","Kältemittel-=-Füllmenge-=-tCO2-Äq.","","","tCO2-Äq.","1.01"]
["","Füllmenge","","","kg","1.50"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6"]
["","Gas","","AD","mm","15.9"]
["","Ableitung","","AD","mm","18"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","20.0"]
["","Wärmeisolierung","","","","Sowohl Flüssigkeits- als auch Gasleitungen"]
["Stromversorgung","Bezeichnung","","","","V3"]
["","Phase","","","","1N~"]
["","Frequenz","","","Hz","50"]
["","Spannung","","","V","230"]
["Strom","Empfohlene Sicherungen","","","A","20"]
["Hinweise","","","","","(1) - Kühlung Ta 35°C - VDWA 18°C (DT = 5°C) - Heizung Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)"]