{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERRQ-AY1"]
[]
[]
[]
[]
["","","","","","ERRQ011AAY1","ERRQ014AAY1","ERRQ016AAY1"]
["Schalldruckpegel","Heizen","","Nom.","dBA","52","53","55"]
["Standardzubehör","Installationsanleitung","","","","1","1","1"]
["Schallleistungspegel","Heizen","","Nom.","dBA","68","69","71"]
["Kältemittel","Charge","","","TCO2-Äquivalent","9.4","9.4","9.4"]
["","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Füllmenge","","","kg","4.5","4.5","4.5"]
["","Typ","","","","R-410A","R-410A","R-410A"]
["Abmessungen","Maßeinheit","","Breite","mm","900","900","900"]
["","","","Tiefe","mm","320","320","320"]
["","","","Höhe","mm","1,345","1,345","1,345"]
["Betriebsbereich","Heizen","","Max.","°C Feuchtkugel","20","20","20"]
["","","","Min.","°C Feuchtkugel","-20","-20","-20"]
["","Warmwasser","","Min.","°C Trockenkugel","-20","-20","-20"]
["","","","Max.","°C Trockenkugel","35","35","35"]
["Gewicht","Maßeinheit","","","kg","120","120","120"]
["Rohrleitungsanschlüsse","Wärmeisolierung","","","","Sowohl Flüssigkeits- als auch Gasleitungen","Sowohl Flüssigkeits- als auch Gasleitungen","Sowohl Flüssigkeits- als auch Gasleitungen"]
["","Flüssigkeit","","AD","mm","9.52","9.52","9.52"]
["","Gas","","AD","mm","15.9","15.9","15.9"]
["","Ableitung","","AD","mm","26x3","26x3","26x3"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","30","30","30"]
["Power supply","Phase","","","","3~","3~","3~"]
["","Frequenz","","","Hz","50","50","50"]
["","Bezeichnung","","","","Y1","Y1","Y1"]
["","Spannung","","","V","380-415","380-415","380-415"]
["Strom","Empfohlene Sicherungen","","","A","16","16","16"]
["Hinweise","","","","","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(2) - Enthält fluorierte Treibhausgase","(2) - Enthält fluorierte Treibhausgase","(2) - Enthält fluorierte Treibhausgase"]