{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSHB16E7"]
[]
[]
[]
[]
["","","","","","ETSHB16P30EG7","ETSHB16P50EG7","ETSHB16P30EF7 (Archived)","ETSHB16P50EF7 (Archived)"]
["Gehäuse","Farbe","","","","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)"]
["","Material","","","","Schlagfestes Polypropylen","Schlagfestes Polypropylen","Schlagfestes Polypropylen","Schlagfestes Polypropylen"]
["Abmessungen","Maßeinheit","","Höhe","mm","1892","1910","1892","1910"]
["","","","Breite","mm","594","792","594","792"]
["","","","Tiefe","mm","644","817","644","816"]
["Gewicht","Maßeinheit","","","kg","76","100","76","100"]
["Schallleistungspegel","Schallleistungspegel-=-Nom.-=-dB(A)","","","dB(A)","45.6","45.6","45.6","45.6"]
["Schalldruckpegel","Nom.","","","dB(A)","32.8","32.8","32.8","32.8"]
["Betriebsbereich","Heizen","Wasserseite","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Kühlen","Umgebung","Min.","°C TK","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Wasserseite","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50"]
["","Spannung","","","V","230","230","230","230"]
["Hinweise","","","","","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897"]
["","","","","","(2) - Siehe Zeichnungen zu Betriebsgrenzen","(2) - Siehe Zeichnungen zu Betriebsgrenzen","(2) - Siehe Zeichnungen zu Betriebsgrenzen","(2) - Siehe Zeichnungen zu Betriebsgrenzen"]