{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / FAA71BUV1B / RZQG100L8Y1B","FAA71BUV1B / FAA71BUV1B / RZQG125L8Y1B","FAA100BUV1B / RZQG100L8Y1B","FAA71BUV1B / RZQG71L8Y1B","FAA100BUV1B / RZQG71L8Y1B"]
["Kühlleistung","Nom.","","kW","","","","6.80","6.80"]
["Raumkühlen","SEER","","","","","","6.43","6.43"]
["","Jährlicher Energieverbrauch","","kWh/a","","","","371","371"]
["","Leistung","Pdesign","kW","","","","6.80","6.80"]
["","Energieeffizienzklasse","","","","","","A++","A++"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","","","","6.33","6.33"]
["","SCOP/A","","","","","","4.02","4.02"]
["","Energieeffizienzklasse","","","","","","A+","A+"]
["","Jährlicher Energieverbrauch","","kWh/a","","","","2,205","2,205"]
["Nominale Effizienz","EER","","","","","","3.40","3.40"]
["","Jährlicher Energieverbrauch","","kWh","","","","1,000"]
["","COP","","","","","","3.70"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","","","A"]
["","","Heizen","","","","","A"]
["Heizleistung","Nom.","","kW","","","","7.50"]
["Energieeffizienzbereich","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Hinweise","","","","","","","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(1) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten"]