{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAQ100CVEB9 / RZQG71L8Y1B","FAQ71CVEB9 / RZQG71L8Y1B","FAQ71CVEB9 / FAQ71CVEB9 / RZQG100L8Y1B","FAQ100CVEB9 / RZQG100L8Y1B","FAQ71CVEB9 / FAQ71CVEB9 / RZQG125L8Y1B"]
["Kühlleistung","Nom.","","kW","","6.8","","9.5"]
["Raumkühlen","SEER","","","6.51","6.43","5.10","6.11","5.10"]
["","Jährlicher Energieverbrauch","","kWh/a","366","371","652","545","824"]
["","Leistung","Pdesign","kW","6.80","6.80","9.50","9.50","12.00"]
["","Energieeffizienzklasse","","","A++","A++","B","A++","B"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","6.33","6.33","11.30","10.20","12.71"]
["","SCOP/A","","","4.02","4.02","3.80","4.01","3.80"]
["","Energieeffizienzklasse","","","A+","A+","A","A+","A"]
["","Jährlicher Energieverbrauch","","kWh/a","2,205","2,205","4,164","3,562","4,683"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","","1,000","","1,315"]
["","EER","","","","3.40","","3.62"]
["","COP","","","","3.70","","3.61"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","A","","A"]
["","","Heizen","","","A","","A"]
["Heizleistung","Nom.","","kW","","7.5","","10.8"]
["Hinweise","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","","(1) - Jährlicher Energieverbrauch gemäß der Energieetikett-Richtlinie 2002/31/EC","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","","(2) - SEER und SCOP gemäß EN 14825","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]