{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FBA71A2VEB / AZAS71M2V1B"]
["Außengerät","","","","AZAS71M2V1B"]
["Kühlleistung","Nom.","","kW","6.80"]
["Heizleistung","Nom.","","kW","7.50"]
["Raumkühlen","Energieeffizienzklasse","","","A"]
["","Leistung","Pdesign","kW","6.80"]
["","SEER","","","5.57"]
["","Jährlicher Energieverbrauch","","kWh/a","427"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A"]
["","Leistung","Pdesign","kW","4.50"]
["","SCOP/A","","","3.81"]
["","Jährlicher Energieverbrauch","","kWh/a","1654"]
["Hinweise","","","","(1) - Kühlen: T2: Innentemp. 26,6 °C TK, 19,4 °C FK, Außentemp. 48 °C TK [Btu/h / W]"]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]