{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":21,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / RZQG71L8Y1B","FCAG100AVEB / RZQG100L8Y1B","FCAG125AVEB / RZQG125L8Y1B","FCAG140AVEB / RZQG100L8Y1B","FCAG140AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG100L8Y1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQG125L8Y1B","FCAG60AVEB / FCAG60AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / RZQG71L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG71L8Y1B","FCAG71AVEB / RZQG71L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG100L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG140L7Y1B","FCAG140AVEB / RZQG140L7Y1B"]
["Kühlleistung","Nom.","","kW","","","","","","","","","","","","","6.80 (1)","","","13.4 (1)","13.4 (1)"]
["Raumkühlen","SEER","","","","","","","","","","","","","5.10","5.10","6.72","","","9.70","6.44"]
["","ηs,c","","%","","","","","","","","","","","","","","","","385.1","254.6"]
["","Jährlicher Energieverbrauch","","kWh/a","","","","","","","","","","","467","467","355","","","829","1,249"]
["","Leistung","Pdesign","kW","","","","","","","","","","","6.80","6.80","6.80","","","13.4","13.4"]
["","Energieeffizienzklasse","","","","","","","","","","","","","A","A","A++"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","","","","","","","","","","","6.00","6.00","6.33","","","12.0","11.6"]
["","SCOP/A","","","","","","","","","","","","","3.80","3.80","4.20","","","3.96","4.27"]
["","Energieeffizienzklasse","","","","","","","","","","","","","A","A","A+"]
["","Jährlicher Energieverbrauch","","kWh/a","","","","","","","","","","","2,211","2,211","2,110","","","4,235","3,795"]
["","ηs,h","","%","","","","","","","","","","","","","","","","155.2","167.6"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","","","","","","","","","","","","","1,005"]
["","EER","","","","","","","","","","","","","","","3.39 (3)","","","4.29 (3)","2.50 (3)"]
["","COP","","","","","","","","","","","","","","","3.97 (3)","","","","3.61 (3)"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","","","","","","","","","","","","A"]
["","","Heizen","","","","","","","","","","","","","","A"]
["Heizleistung","Nom.","","kW","","","","","","","","","","","","","7.50 (2)","","","15.5 (2)","15.5 (2)"]
["Hinweise","","","","","","","","","","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m; Niveauunterschied: 0 m","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m; Niveauunterschied: 0 m","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m; Niveauunterschied: 0 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m; Niveauunterschied: 0 m"]
["","","","","","","","","","","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 7,5 m; Niveauunterschied: 0 m","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 7,5 m; Niveauunterschied: 0 m","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 7,5 m; Niveauunterschied: 0 m","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 7,5 m; Niveauunterschied: 0 m"]
["","","","","","","","","","","","","","","(3) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","(3) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","","(3) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","(3) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["Energieeffizienzbereich","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","A+++ ~ D","A+++ ~ D"]
["Außengerät","","","","","","","","","","","","","","","","","RZQG100L8Y1","RZQG125L8Y1"]
["Raumkühlen","Energieeffizienzklasse","","","","","","","","","","","","","","","","A","A"]
["","Leistung","Pdesign","kW","","","","","","","","","","","","","","9.50","12.0"]
["","SEER","","","","","","","","","","","","","","","","5.10","5.10"]
["","Jährlicher Energieverbrauch","","kWh/a","","","","","","","","","","","","","","652","824"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","","","","","","","","","","","","","","A","A"]
["","Leistung","Pdesign","kW","","","","","","","","","","","","","","11.3","12.7"]
["","SCOP/A","","","","","","","","","","","","","","","","3.80","3.80"]
["","Jährlicher Energieverbrauch","","kWh/a","","","","","","","","","","","","","","4164","4683"]