{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":24,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / RZQG71L9V1B","FCAG100AVEB / RZQG100L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG125L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L9V1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQG125L9V1B","FCAG50AVEB / FCAG50AVEB / RZQG100L9V1B","FCAG60AVEB / FCAG60AVEB / RZQG125L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG71L9V1B","FCAG35AVEB / FCAG35AVEB / RZQG71L9V1B","FCAG50AVEB / FCAG50AVEB / RZQG71L9V1B","FCAG71AVEB / RZQG71L9V1B","FCAG140AVEB / RZQG100L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L9V1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQG100L9V1B","FCAG71AVEB / FCAG71AVEB / RZQG100L9V1B","FCAG140AVEB / RZQG125L9V1B","FCAG125AVEB / RZQG125L9V1B","FCAG71AVEB / FCAG71AVEB / RZQG125L9V1B","FCAG140AVEB / RZQG140L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG140L9V1B"]
["Energieeffizienzbereich","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Raumkühlen","SEER","","","","","","","","","","5.10","5.10","5.10","6.72","6.80","","","","6.00","6.00","5.10","6.44","9.70"]
["","Jährlicher Energieverbrauch","","kWh/a","","","","","","","","467","467","467","355","489","","","","700","700","824","1,249","829"]
["","Leistung","Pdesign","kW","","","","","","","","6.80","6.80","6.80","6.80","9.50","","","","12.00","12.0","12.0","13.4","13.4"]
["","Energieeffizienzklasse","","","","","","","","","","A","A","A","A++","A++","","","","A+","A+","A"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","","","","","","","","6.00","6.00","6.00","6.33","11.30","","","","12.66","12.7","12.7","11.6","12.0"]
["","SCOP/A","","","","","","","","","","3.80","3.80","3.80","4.20","4.61","","","","4.10","4.10","3.80","4.27","3.96"]
["","Energieeffizienzklasse","","","","","","","","","","A","A","A","A+","A++","","","","A+","A+","A"]
["","Jährlicher Energieverbrauch","","kWh/a","","","","","","","","2,211","2,211","2,211","2,110","3,432","","","","4,323","4,323","4,683","3,795","4,235"]
["Hinweise","","","","","","","","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m; Niveauunterschied: 0 m","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m; Niveauunterschied: 0 m","","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m; Niveauunterschied: 0 m","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m; Niveauunterschied: 0 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m; Niveauunterschied: 0 m"]
["","","","","","","","","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 7,5 m; Niveauunterschied: 0 m","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 7,5 m; Niveauunterschied: 0 m","","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 7,5 m; Niveauunterschied: 0 m","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 7,5 m; Niveauunterschied: 0 m","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 7,5 m; Niveauunterschied: 0 m"]
["","","","","","","","","","","","","(3) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","(3) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","","","","","(3) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","(3) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","(3) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["Kühlleistung","Nom.","","kW","","","","","","","","","","","6.80 (1)","","","","","","12.0 (1)","","13.4 (1)","13.4 (1)"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","","","","","","","","","","","1,005","","","","","","1,610"]
["","EER","","","","","","","","","","","","","3.39 (3)","","","","","","3.73 (3)","","2.50 (3)","4.29 (3)"]
["","COP","","","","","","","","","","","","","3.97 (3)","","","","","","3.63 (3)","","3.61 (3)"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","","","","","","","","","","A","","","","","","A"]
["","","Heizen","","","","","","","","","","","","A","","","","","","A"]
["Heizleistung","Nom.","","kW","","","","","","","","","","","7.50 (2)","","","","","","13.5 (2)","","15.5 (2)","15.5 (2)"]
["Außengerät","","","","","","","","","","","","","","","","RZQG100L9V1","RZQG100L9V1","RZQG100L9V1"]
["Raumkühlen","Energieeffizienzklasse","","","","","","","","","","","","","","","A","A","A"]
["","Leistung","Pdesign","kW","","","","","","","","","","","","","9.50","9.50","9.50"]
["","SEER","","","","","","","","","","","","","","","5.10","5.10","5.10"]
["","Jährlicher Energieverbrauch","","kWh/a","","","","","","","","","","","","","652","652","652"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","","","","","","","","","","","","","A","A","A"]
["","Leistung","Pdesign","kW","","","","","","","","","","","","","7.60","11.3","11.3"]
["","SCOP/A","","","","","","","","","","","","","","","3.80","3.80","3.80"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","","","","","","","","","","","","","6.95"]
["","Jährlicher Energieverbrauch","","kWh/a","","","","","","","","","","","","","4164","4164","4164"]
["Raumkühlen","ηs,c","","%","","","","","","","","","","","","","","","","","","","254.6","385.1"]
["Raumheizen (Durchschnittliches Klima)","ηs,h","","%","","","","","","","","","","","","","","","","","","","167.6","155.2"]