{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L"]
[]
[]
[]
[]
["","","","","FCAG50BVEB / RXS50L2V1B","FCAG60BVEB / RXS60L2V1B"]
["Kühlleistung","Nom.","","kW","5.00","5.70"]
["Heizleistung","Nom.","","kW","6.00","7.00"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","705","820"]
["","COP","","","3.70","3.52"]
["","EER","","","3.55","3.48"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A"]
["","","Heizen","","A","B"]
["Piping connections","Drain","OD","mm","VP25 (Außendurchmesser 32, Innendurchmesser 25)","VP25 (Außendurchmesser 32, Innendurchmesser 25)"]
["","Gas","AD","mm","12.70","12.70"]
["","Flüssigkeit","AD","mm","6.35","6.35"]
["Hinweise","","","","(1) - Bei normalem Betrieb: +22 °C / + 32 °C","(1) - Bei normalem Betrieb: +22 °C / + 32 °C"]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten","(4) - Siehe separate Zeichnung für die elektrischen Daten"]