{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":8,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-F"]
[]
[]
[]
[]
["","","","","FCAHG100FVEB","FCAHG125FVEB","FCAHG140FVEB","FCAHG71FVEB"]
["Schalldruckpegel","Heizen","Hoch","dBA","44","45","45"]
["","","Mittel","dBA","39","40","41"]
["","","Niedrig","dBA","33","35","37"]
["","Kühlen","Mittel","dBA","39","40","41"]
["","","Niedrig","dBA","33","35","37"]
["","","Hoch","dBA","44","45","45"]
["Standardzubehör","Installations- und Bedienungsanleitung","","","Installations- und Bedienungsanleitung","Installations- und Bedienungsanleitung","Installations- und Bedienungsanleitung","Installations- und Bedienungsanleitung"]
["","Installationsanleitung","","","Installationsanleitung","Installationsanleitung","Installationsanleitung","Installationsanleitung"]
["Kältemittel","GWP","","","675","675","675","675"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","9.52","9.52","9.52","9.52"]
["","Gas","AD","mm","15.9","15.9","15.9"]
["","Ableitung","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Geräteblende 4","Abmessungen","Tiefe","mm","950","950","950","950"]
["","","Breite","mm","950","950","950","950"]
["","","Höhe","mm","50","50","50","50"]
["","Modell","","","BYCQ140D7W1 – Weiß mit grauen Lamellen","BYCQ140D7W1 – Weiß mit grauen Lamellen","BYCQ140D7W1 – Weiß mit grauen Lamellen","BYCQ140D7W1 – Weiß mit grauen Lamellen"]
["","Farbe","","","Reinweiß (RAL 9010)","Reinweiß (RAL 9010)","Reinweiß (RAL 9010)","Reinweiß (RAL 9010)"]
["","Gewicht","","kg","5.4","5.4","5.4","5.4"]
["Schallleistungspegel","Kühlen","","dBA","61","61","61"]
["","Heizen","","dBA","61","61","61"]
["Abmessungen","Maßeinheit","Breite","mm","840","840","840","840"]
["","","Tiefe","mm","840","840","840","840"]
["","","Höhe","mm","288","288","288","288"]
["Gehäuse","Material","","","Galvanisiertes Stahlblech.","Galvanisiertes Stahlblech.","Galvanisiertes Stahlblech.","Galvanisiertes Stahlblech."]
["Gewicht","Maßeinheit","","kg","26.0","26.0","26.0","25.0"]
["Geräteblende","Gewicht","","kg","10","10","10"]
["","Modell","","","BYCQ140D7GFW1 – selbstreinigende Zierblende mit feinmaschigem Filter","BYCQ140D7GFW1 – selbstreinigende Zierblende mit feinmaschigem Filter","BYCQ140D7GFW1 – selbstreinigende Zierblende mit feinmaschigem Filter"]
["","Abmessungen","Höhe","mm","130","130","130"]
["","","Tiefe","mm","950","950","950"]
["","","Breite","mm","950","950","950"]
["","Farbe","","","Reinweiß (RAL 9010)","Reinweiß (RAL 9010)","Reinweiß (RAL 9010)"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Frequenz","","Hz","50/60","50/60","50/60","50/60"]
["","Bezeichnung","","","VE","VE","VE","VE"]
["","Spannung","","V","220-240","220-240","220-240","220-240"]
["Hinweise","","","","(1) - Das BYCQ140D7W1W verfügt über eine weiße Isolation. Beachten Sie, dass Schmutz auf weißem Isolationsmaterial stärker zu sehen ist und daher eine Installation der Zierblende BYCQ140D7W1W in staubreichen Umgebungen nicht empfehlenswert ist.","(1) - Das BYCQ140D7W1W verfügt über eine weiße Isolation. Beachten Sie, dass Schmutz auf weißem Isolationsmaterial stärker zu sehen ist und daher eine Installation der Zierblende BYCQ140D7W1W in staubreichen Umgebungen nicht empfehlenswert ist.","(1) - Das BYCQ140D7W1W verfügt über eine weiße Isolation. Beachten Sie, dass Schmutz auf weißem Isolationsmaterial stärker zu sehen ist und daher eine Installation der Zierblende BYCQ140D7W1W in staubreichen Umgebungen nicht empfehlenswert ist.","(1) - Das BYCQ140D7W1W verfügt über eine weiße Isolation. Beachten Sie, dass Schmutz auf weißem Isolationsmaterial stärker zu sehen ist und daher eine Installation der Zierblende BYCQ140D7W1W in staubreichen Umgebungen nicht empfehlenswert ist."]
["","","","","(2) - Enthält fluorierte Treibhausgase","(2) - Enthält fluorierte Treibhausgase","(2) - Enthält fluorierte Treibhausgase","(2) - Enthält fluorierte Treibhausgase"]
["","","","","(3) - Der Schallleistungspegel ist ein absoluter Wert und gibt die \"Leistung\" an, die eine Schallquelle erzeugt.","(3) - Der Schallleistungspegel ist ein absoluter Wert und gibt die \"Leistung\" an, die eine Schallquelle erzeugt.","(3) - Der Schallleistungspegel ist ein absoluter Wert und gibt die \"Leistung\" an, die eine Schallquelle erzeugt.","(3) - Der Schallleistungspegel ist ein absoluter Wert und gibt die \"Leistung\" an, die eine Schallquelle erzeugt."]
["Schalldruckpegel","Heizen","Hoch","dBA","","","","36"]
["","","Mittel","dBA","","","","33"]
["","","Niedrig","dBA","","","","29"]
["","Kühlen","Mittel","dBA","","","","33"]
["","","Niedrig","dBA","","","","29"]
["","","Hoch","dBA","","","","36"]
["Rohrleitungsanschlüsse","Gas","AD","mm","","","","15.9"]
["","Ableitung","","","","","","VP25 (I.D. 25/O.D. 32)"]
["Schallleistungspegel","Kühlen","","dBA","","","","53"]
["","Heizen","","dBA","","","","53"]
["Geräteblende","Gewicht","","kg","","","","10"]
["","Modell","","","","","","BYCQ140D7GFW1 – selbstreinigende Zierblende mit feinmaschigem Filter"]
["","Abmessungen","Höhe","mm","","","","130"]
["","","Tiefe","mm","","","","950"]
["","","Breite","mm","","","","950"]
["","Farbe","","","","","","Reinweiß (RAL 9010)"]