{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":21,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FCQG100FVEB / RZQG71L9V1B","FCQG35FVEB / FCQG35FVEB / RZQG71L9V1B","FCQG71FVEB / RZQG71L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L9V1B","FCQG71FVEB / FCQG71FVEB / RZQG100L9V1B","FCQG100FVEB / RZQG100L9V1B","FCQG140FVEB / RZQG100L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L9V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG100L9V1B","FCQG50FVEB / FCQG50FVEB / RZQG100L9V1B","FCQG71FVEB / FCQG71FVEB / RZQG125L9V1B","FCQG125FVEB / RZQG125L9V1B","FCQG140FVEB / RZQG125L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG125L9V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG125L9V1B","FCQG60FVEB / FCQG60FVEB / RZQG125L9V1B","FCQG140FVEB / RZQG140L9V1B"]
["Kühlleistung","Nom.","","kW","","","6.8","","","9.5","","","","","","12.0","","","","","13.4"]
["Raumkühlen","SEER","","","6.80","5.10","6.72","5.10","5.10","6.80","6.80","5.10","5.10","5.10","5.10","6.00","6.00","5.10","5.10","5.10"]
["","Jährlicher Energieverbrauch","","kWh/a","350","467","355","652","652","489","489","652","652","652","824","700","700","824","824","824"]
["","Leistung","Pdesign","kW","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00","12.00"]
["","Energieeffizienzklasse","","","A++","B","A++","B","B","A++","A++","B","B","B","B","A+","A+","B","B","B"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","6.33","6.00","6.33","11.30","11.30","11.30","11.30","11.30","11.30","11.30","12.71","12.66","12.66","12.71","12.71","12.71"]
["","SCOP/A","","","4.20","3.80","4.20","3.80","3.80","4.61","4.61","3.80","3.80","3.80","3.80","4.10","4.10","3.80","3.80","3.80"]
["","Energieeffizienzklasse","","","A+","A","A+","A","A","A++","A++","A","A","A","A","A+","A+","A","A","A"]
["","Jährlicher Energieverbrauch","","kWh/a","2,110","2,211","2,110","4,164","4,164","3,432","3,432","4,164","4,164","4,164","4,683","4,323","4,323","4,683","4,683","4,683"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","","","1,005","","","1,225","","","","","","1,610"]
["","EER","","","","","3.39","","","3.87","","","","","","3.73","","","","","3.21"]
["","COP","","","","","3.97","","","4.15","","","","","","3.63","","","","","3.61"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","","A","","","A","","","","","","A"]
["","","Heizen","","","","A","","","A","","","","","","A"]
["Heizleistung","Nom.","","kW","","","7.5","","","10.8","","","","","","13.5","","","","","15.5"]
["Hinweise","","","","","","(1) - Jährlicher Energieverbrauch gemäß der Energieetikett-Richtlinie 2002/31/EC","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","","","(2) - SEER und SCOP gemäß EN 14825","","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast","","","","","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast","","","","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]
["","","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]