{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDA125A5VEB / RZQG125L8Y1B"]
["Kühlleistung","Nom.","","kW","12.00"]
["Raumkühlen","SEER","","","5.81"]
["","Jährlicher Energieverbrauch","","kWh/a","723"]
["","Leistung","Pdesign","kW","12.00"]
["","Energieeffizienzklasse","","","A+"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","12.71"]
["","SCOP/A","","","4.21"]
["","Energieeffizienzklasse","","","A+"]
["","Jährlicher Energieverbrauch","","kWh/a","4,227"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","1,600"]
["","EER","","","3.75"]
["","COP","","","3.83"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A"]
["","","Heizen","","A"]
["Heizleistung","Nom.","","kW","13.50"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten"]