{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RR-BW1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9/RR125B8W1B"]
["Kühlleistung","Nom.","","kW","12.5 (1)"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","9.52"]
["","Gas","AD","mm","15.9"]
["","Ableitung","AD","mm","26"]
["Nominale Effizienz","EER","","","2.61"]
["","Jährlicher Energieverbrauch","","kWh","2,395"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","D"]
["Hinweise","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m; Niveauunterschied: 0 m"]
["","","","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]