{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Schalldruckpegel","Heizen","","Hoch","dBA","35.0","35.0","","38.0"]
["","","","Mittel","dBA","33.0","33.0","","35.0"]
["","","","Niedrig","dBA","27.0","27.0","","30.0"]
["","Kühlen","","Mittel","dBA","33.0","33.0","","35.0"]
["","","","Niedrig","dBA","27.0","27.0","","30.0"]
["","","","Hoch","dBA","35.0","35.0","","38.0"]
["Standardzubehör","Installationsanleitung","","","","1","1","","1"]
["","Bedienungsanleitung","","","","1","1","","1"]
["","Isolierung für die Armatur","","","","1","1","","1"]
["","Dichtungsmatte","","","","1","1","","1"]
["","Klemmblech","","","","1","1","","1"]
["","Kondensatschlauch","","","","1","1","","1"]
["","Unterlegscheibe für Aufhängung","","","","8","8","","8"]
["","Dichtungsmaterial","","","","2","2","","2"]
["","Klemmen","","","","6","6","","6"]
["","Unterlegscheibe für Befestigungsplatte","","","","4","4","","4"]
["","Schrauben für Kanalflansche","","","","1","1","","1"]
["","Luftfilter","","","","1","1","","1"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35","","6.35"]
["","Gas","","AD","mm","9.50","9.50","","12.70"]
["","Ableitung","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Leistungsaufnahme","Kühlen","","Nom.","kW","0.036","0.036","","0.060"]
["","Heizen","","Nom.","kW","0.036","0.036","","0.060"]
["Sound power level","Kühlen","","","dBA","53.0","53.0","","56.0"]
["","Heizen","","","dBA","53.0","53.0","","56.0"]
["Abmessungen","Maßeinheit","","Breite","mm","750","750","","1,150"]
["","","","Tiefe","mm","620","620","","620"]
["","","","Höhe","mm","200","200","","200"]
["Gewicht","Maßeinheit","","","kg","21","21","","28"]
["Ventilator","Externer statischer Druck","","Nom.","Pa","30","30","","40"]
["","Luftstromvolumen","Heizen","Hoch","m³/min","8.7","8.7","","16.0"]
["","","","Mittel","m³/min","8.0","8.0","","14.8"]
["","","","Niedrig","m³/min","7.3","7.3","","13.5"]
["","","Kühlen","Niedrig","m³/min","7.3","7.3","","13.5"]
["","","","Mittel","m³/min","8.0","8.0","","14.8"]
["","","","Hoch","m³/min","8.7","8.7","","16.0"]
["Power supply","Phase","","","","1~","1~","","1~"]
["","Frequenz","","","Hz","50","50","","50"]
["","Spannung","","","V","220-240","220-240","","220-240"]
["Hinweise","","","","","(1) - Siehe separate Zeichnung für die elektrischen Daten","(1) - Siehe separate Zeichnung für die elektrischen Daten","","(1) - Siehe separate Zeichnung für die elektrischen Daten"]
["Leistungsaufnahme","Kühlen","","Nom.","kW","","","0.060"]
["","Heizen","","Nom.","kW","","","0.060"]
["Abmessungen","Maßeinheit","","Höhe","mm","","","200"]
["","","","Breite","mm","","","1150"]
["","","","Tiefe","mm","","","620"]
["Gewicht","Maßeinheit","","","kg","","","28"]
["Ventilator","Luftstromvolumen","Kühlen","Hoch","m³/min","","","15.8"]
["","","","Mittel","m³/min","","","14.6"]
["","","","Niedrig","m³/min","","","13.3"]
["","","Heizen","Hoch","m³/min","","","15.8"]
["","","","Mittel","m³/min","","","14.6"]
["","","","Niedrig","m³/min","","","13.3"]
["","Externer statischer Druck","","Nom.","Pa","","","40"]
["Schallleistungspegel","Kühlung","","","dBA","","","55.0"]
["","Heizen","","","dBA","","","55.0"]
["Schalldruckpegel","Kühlen","","Hoch","dBA","","","38.0"]
["","","","Mittel","dBA","","","35.0"]
["","","","Niedrig","dBA","","","30.0"]
["","Heizen","","Hoch","dBA","","","38.0"]
["","","","Mittel","dBA","","","35.0"]
["","","","Niedrig","dBA","","","30.0"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","","6.35"]
["","Gas","","AD","mm","","","12.70"]
["","Ableitung","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Standardzubehör","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Luftfilter","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Stromversorgung","Phase","","","","","","1~"]
["","Frequenz","","","Hz","","","50"]
["","Spannung","","","V","","","220-240"]