{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-E / RXS-K"]
[]
[]
[]
[]
["","","","","FDXS25E7VMB / RXS25K2V1B"]
["Kühlleistung","Nom.","","kW","2.40 (3)"]
["Piping connections","Flüssigkeit","AD","mm","6.35"]
["","Gas","AD","mm","9.5"]
["","Drain","OD","mm","VP20 (Außendurchmesser 26, Innendurchmesser 20)"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","345"]
["","EER","","","3.48"]
["","COP","","","3.52"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A"]
["","","Heizen","","B"]
["Heizleistung","Nom.","","kW","3.20 (4)"]
["Hinweise","","","","(1) - Energieetikett: Skala von A (am effizientesten) bis G (am wenigsten effizient)"]
["","","","","(2) - Jährlicher Energieverbrauch: auf der Grundlage von etwa 500 Betriebsstunden pro Jahr bei Volllast (Nennbedingungen)"]
["","","","","(3) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, äquivalente Leitungslänge: 5 m; Niveauunterschied: 0 m"]
["","","","","(4) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m"]
["","","","","(5) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]