{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-A"]
[]
[]
[]
[]
["","","","","FFA50A2VEB9 / RXM50A5V1B"]
["Kühlleistung","Nom.","","kW","5.00"]
["Heizleistung","Nom.","","kW","5.80"]
["Nominale Effizienz","EER","","","3.24"]
["","COP","","","3.49"]
["","Jährlicher Energieverbrauch","","kWh","772"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A"]
["","","Heizen","","B"]
["Raumkühlen","Energieeffizienzklasse","","","A+"]
["","Leistung","Pdesign","kW","5.00"]
["","SEER","","","5.98"]
["","Jährlicher Energieverbrauch","","kWh/a","293"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A"]
["","Leistung","Pdesign","kW","3.84"]
["","SCOP/A","","","3.90"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung&nbsp;Pdh bei&nbsp;-10°-=-kW","","kW","3.40"]
["","Jährlicher Energieverbrauch","","kWh/a","1378"]