{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-B9V / RXS-F"]
[]
[]
[]
[]
["","","","","FFQ60B9V1B / RXS60F3V1B","FFQ60B9V1B / RXS60F4V1B"]
["Kühlleistung","Nom.","","kW","5.80 (3)","5.80 (3)"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","1,035","1,035"]
["","EER","","","2.80","2.80"]
["","COP","","","2.81","2.81"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","D","D"]
["","","Heizen","","D","D"]
["Heizleistung","Nom.","","kW","7.00 (4)","7.00 (4)"]
["Hinweise","","","","(1) - Energieetikett: Skala von A (am effizientesten) bis G (am wenigsten effizient)","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","(2) - Jährlicher Energieverbrauch: auf der Grundlage von etwa 500 Betriebsstunden pro Jahr bei Volllast (Nennbedingungen)","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]
["","","","","(3) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 7,5 m; Niveauunterschied: 0 m"]
["","","","","(4) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 7,5 m; Niveauunterschied: 0 m"]
["","","","","(5) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]