{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":23,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ100CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ50CBVEB / FHQ50CBVEB / RZQG71L8Y1B","FHQ71CBVEB / RZQG71L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG100L8Y1B","FHQ100CBVEB / RZQG100L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG100L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / RZQG100L8Y1B","FHQ140CBVEB / RZQG125L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG125L8Y1B","FHQ125CBVEB / RZQG125L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQG125L8Y1B","FHQ60CBVEB / FHQ60CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG140L7Y1B"]
["Kühlleistung","Nom.","","kW","","","","","6.8","","","","9.5","","","","","","","12.0","","","13.4"]
["Raumkühlen","SEER","","","6.95","5.10","5.10","5.10","6.86","5.10","6.11","5.10","6.11","5.10","5.10","5.10","5.10","6.01","5.10","6.01","5.10","5.10"]
["","Jährlicher Energieverbrauch","","kWh/a","343","467","467","467","347","824","545","652","545","652","652","652","652","699","824","699","824","824"]
["","Leistung","Pdesign","kW","6.80","6.80","6.80","6.80","6.80","12.00","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00"]
["","Energieeffizienzklasse","","","A++","B","B","B","A++","B","A++","B","A++","B","B","B","B","A+","B","A+","B","B"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","7.60","6.00","6.00","6.00","7.60","12.71","11.30","11.30","11.30","11.30","11.30","11.30","11.30","14.13","12.71","14.13","12.71","12.71"]
["","SCOP/A","","","4.32","3.80","3.80","3.80","4.32","3.80","4.61","3.80","4.61","3.80","3.80","3.80","3.80","4.23","3.80","4.23","3.80","3.80"]
["","Energieeffizienzklasse","","","A+","A","A","A","A+","A","A++","A","A++","A","A","A","A","A+","A","A+","A","A"]
["","Jährlicher Energieverbrauch","","kWh/a","2,463","2,211","2,211","2,211","2,463","4,683","3,432","4,164","3,432","4,164","4,164","4,164","4,164","4,677","4,683","4,677","4,683","4,683"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","","","","","890","","","","1,245","","","","","","","1,790","","","2,025"]
["","EER","","","","","","","3.82","","","","3.81","","","","","","","3.35","","","3.31"]
["","COP","","","","","","","4.13","","","","4.15","","","","","","","3.89","","","3.63"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","","","","A","","","","A","","","","","","","A","","","A"]
["","","Heizen","","","","","","A","","","","A","","","","","","","A","","","A"]
["Heizleistung","Nom.","","kW","","","","","7.5","","","","10.8","","","","","","","13.5","","","15.5"]
["Hinweise","","","","","","","","(1) - Jährlicher Energieverbrauch gemäß der Energieetikett-Richtlinie 2002/31/EC","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","","","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","","","","","(2) - SEER und SCOP gemäß EN 14825","","","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast","","","","","","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast","","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]