{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Schalldruckpegel","Heizen","Hoch","dBA","46"]
["","","Flüsterbetrieb","dBA","30"]
["","","Niedrig","dBA","33"]
["","Kühlen","Flüsterbetrieb","dBA","29"]
["","","Niedrig","dBA","32"]
["","","Hoch","dBA","38"]
["","","Nom.","dBA","36"]
["","Kühlen","Nom.","dBA","35"]
["Standardzubehör","Installationsanleitung","","","1"]
["","Bedienungsanleitung","","","1"]
["","Infrarot-Fernbedienung","","","1"]
["","Trockenbatterien, Typ AAA","","","2"]
["","Fernbedienungshalterung","","","1"]
["","Montageplatte","","","1"]
["","Wärmeisolierungsrohr (Kältemittelleitung)","","","8"]
["","Luftreinigungsfilter","","","1"]
["","Photokatalytischer Geruchsfilter","","","1"]
["","Seitliche Abdeckung","","","2"]
["","Dichtungsband","","","4"]
["Control systems","Infrared remote control","","","ARC433B67"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","6.35"]
["","Gas","AD","mm","9.5"]
["","Ableitung","","","18"]
["Schallleistungspegel","Kühlen","","dBA","53"]
["","Heizen","","dBA","59"]
["Abmessungen","Maßeinheit","Breite","mm","1,050"]
["","","Tiefe","mm","200"]
["","","Höhe","mm","490"]
["Gehäuse","Colour","","","Mandelweiß"]
["Gewicht","Maßeinheit","","kg","16"]
["Power supply","Phase","","","1~"]
["","Frequenz","","Hz","50"]
["","Bezeichnung","","","VM"]
["","Spannung","","V","220-240"]
["Hinweise","","","","(1) - 220 V"]
["","","","","(2) - 230 V"]
["","","","","(3) - 240 V"]
["","","","","(4) - Bei Anschluss an einem Multi-Außengerät lesen Sie bitte die technischen Gerätedaten des anzuschließenden Multi-Außengeräts."]