{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":11,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B"]
["Kühlleistung","Nom.","","kW","4.00","4.00","4.0","5.20","4.00","4.00","6.00"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","467","482","482","593","471","457","787"]
["","EER","","","4.28","4.15","4.15","4.38","4.25","4.38","3.81"]
["","COP","","","4.32","3.95","3.95","4.42","4.05","4.04","3.88"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A","A","A","A","A","A"]
["","","Heizen","","A","A","A","A","A","A","A"]
["Heizleistung","Nom.","","kW","4.60","4.60","4.60","6.80","6.80","6.50","7.80"]
["Hinweise","","","","","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m. Daten für Baureihe mit Standard-Wirkungsgrad. Toleranzen Eurovent 2015 werden verwendet."]
["","","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten"]