{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Schalldruckpegel","Heizen","","Hoch","dBA","38","39","42","42","44","","46"]
["","","","Flüsterbetrieb","dBA","25","25","26","30","31","","34"]
["","","","Niedrig","dBA","28","28","29","33","34","","37"]
["","Kühlen","","Flüsterbetrieb","dBA","22","22","23","30","31","","34"]
["","","","Niedrig","dBA","25","25","26","33","34","","37"]
["","","","Hoch","dBA","38","38","42","42","43","","46"]
["","","","Nom.","dBA","33","34","36","38","39","","42"]
["","Kühlen","","Nom.","dBA","32","32","34","38","39","","42"]
["Standardzubehör","Fotokatalytischer Luftreinigungsfilter mit Titanapatit","","","","2","2","2","2","2"]
["","Bedienungsanleitung","","","","1","1","1","1","1","","1"]
["","Installationsanleitung","","","","1","1","1","1","1","","1"]
["","Infrarotfernbedienung","","","","1","1","1","1","1","","1"]
["","Batterien","","","","2","2","2","2","2","","2"]
["","Fernbedienungshalterung","","","","1","1","1","1","1","","1"]
["","Befestigungsschrauben für Hauptgerät","","","","2","2","2","2","2","","2"]
["","Montageplatte","","","","1","1","1","1","1","","1"]
["Control systems","Infrared remote control","","","","","","","","","","ARC452A3"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Gas","","AD","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Ableitung","","","","18","18","18","18","18","","18"]
["Leistungsaufnahme","Kühlen","","Nom.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Heizen","","Nom.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Schallleistungspegel","Kühlen","","","dBA","54","54","58","58","59","","63"]
["","Heizen","","","dBA","54","55","58","58","60","","62"]
["Abmessungen","Maßeinheit","","Breite","mm","800","800","800","800","800","","1,050"]
["","","","Tiefe","mm","215","215","215","215","215","","250"]
["","","","Höhe","mm","295","295","295","295","295","","290"]
["Gehäuse","Colour","","","","Weiß","Weiß","Weiß","Weiß","Weiß","","Weiß"]
["Gewicht","Maßeinheit","","","kg","9","9","10","10","10","","12"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","","1~"]
["","Frequenz","","","Hz","50","50","50","50","50","","50"]
["","Bezeichnung","","","","V1","V1","V1","V1","V1","","V1"]
["","Spannung","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Hinweise","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - SL: Die flüsterleise Ventilatorstufe der Luftmengeneinstellung."]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 220 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 230 V"]
["Ventilator","Luftstromvolumen","Kühlen","Nom.","m³/min","","","","","","16.0"]
["Schalldruckpegel","Kühlen","","Nom.","dBA","","","","","","41"]
["Ventilator","Luftstromvolumen","Heizen","Nom.","m³/min","","","","","","14.9"]
["Schalldruckpegel","Heizen","","Nom.","dBA","","","","","","40"]
["Leistungsaufnahme","Kühlen","","Nom.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Heizen","","Nom.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Gehäuse","Farbe","","","","","","","","","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","","","","","","290"]
["","","","Breite","mm","","","","","","1050"]
["","","","Tiefe","mm","","","","","","250"]
["Gewicht","Maßeinheit","","","kg","","","","","","12"]
["Ventilator","Luftstromvolumen","Kühlen","Hoch","m³/min","","","","","","16.0"]
["","","","Niedrig","m³/min","","","","","","11.3"]
["","","","Flüsterbetrieb","m³/min","","","","","","10.1"]
["","","Heizen","Hoch","m³/min","","","","","","17.2"]
["","","","Niedrig","m³/min","","","","","","12.6"]
["","","","Flüsterbetrieb","m³/min","","","","","","11.3"]
["Schallleistungspegel","Kühlung","","","dBA","","","","","","60"]
["","Heizen","","","dBA","","","","","","59"]
["Schalldruckpegel","Kühlen","","Hoch","dBA","","","","","","45"]
["","","","Niedrig","dBA","","","","","","36"]
["","","","Flüsterbetrieb","dBA","","","","","","33"]
["","Heizen","","Hoch","dBA","","","","","","44"]
["","","","Niedrig","dBA","","","","","","35"]
["","","","Flüsterbetrieb","dBA","","","","","","32"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","","","","","6.35"]
["","Gas","","AD","mm","","","","","","12.7"]
["","Ableitung","","","","","","","","","18"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","","","","","","ARC452A3"]
["Standardzubehör","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Stromversorgung","Bezeichnung","","","","","","","","","V1"]
["","Phase","","","","","","","","","1~"]
["","Frequenz","","","Hz","","","","","","50"]
["","Spannung","","","V","","","","","","220-240"]
["Standardzubehör","Fotokatalytischer Luftreinigungsfilter mit Titanapatit ohne Rahmen","","","","","","","","","","2"]
["Hinweise","","","","","","","","","","","(4) - 240 V"]