{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":5,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-AW"]
[]
[]
[]
[]
["","","","","FTXTA30A2V1BW"]
["Schalldruckpegel","Heizen","Hoch","dBA","41"]
["","","Mittel","dBA","31"]
["","","Flüsterbetrieb","dBA","19"]
["","","Niedrig","dBA","24"]
["","Kühlen","Mittel","dBA","32"]
["","","Flüsterbetrieb","dBA","20"]
["","","Niedrig","dBA","25"]
["","","Hoch","dBA","43"]
["Standardzubehör","Installationsanleitung","","","1"]
["","Bedienungsanleitung","","","1"]
["","Luftfilter","","","2"]
["","Infrarot-Fernbedienung","","","1"]
["","Montageplatte für Fernbedienung","","","1"]
["","Schraubensack","","","1"]
["","Schraubenabdeckung","","","2"]
["","Trockenbatterien, Typ AAA","","","2"]
["","Allgemeine Schutzmaßnahmen","","","1"]
["Kältemittel","GWP","","","675.0"]
["Regelungssysteme","Verkabelte Fernbedienung","","","BRC073A4"]
["","Infrared remote control","","","ARC466A59"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","6.35"]
["","Gas","AD","mm","9.50"]
["","Ableitung","","","18"]
["Leistungsaufnahme","Kühlen","Nom.","kW","0.023"]
["","Heizen","Nom.","kW","0.022"]
["Schallleistungspegel","Kühlen","","dBA","60"]
["","Heizen","","dBA","60"]
["Abmessungen","Maßeinheit","Breite","mm","798"]
["","","Tiefe","mm","189"]
["","","Höhe","mm","295"]
["Gehäuse","Colour","","","Weiß"]
["Gewicht","Maßeinheit","","kg","11.5"]
["Power supply","Phase","","","1~"]
["","Frequenz","","Hz","50"]
["","Bezeichnung","","","V1"]
["","Spannung","","V","220-240"]