{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A"]
[]
[]
[]
[]
["","","","","","FTXTM30A2V1B","FTXTM40A2V1B"]
["Leistungsaufnahme","Kühlen","","Nom.","kW","0.029","0.053"]
["","Heizen","","Nom.","kW","0.024","0.06"]
["Gehäuse","Farbe","","","","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","298","298"]
["","","","Breite","mm","804","997"]
["","","","Tiefe","mm","252","292"]
["Gewicht","Maßeinheit","","","kg","12","15"]
["Ventilator","Luftstromvolumen","Kühlen","Hoch","m³/min","13.2","15.1"]
["","","","Mittel","m³/min","8.1","9.2"]
["","","","Niedrig","m³/min","5.6","5.6"]
["","","","Flüsterbetrieb","m³/min","4.8","4.8"]
["","","Heizen","Hoch","m³/min","11.7","17"]
["","","","Mittel","m³/min","7.7","10"]
["","","","Niedrig","m³/min","5.6","6"]
["","","","Flüsterbetrieb","m³/min","4.7","5.1"]
["Schallleistungspegel","Kühlung","","","dBA","60","60"]
["","Heizen","","","dBA","59","60"]
["Schalldruckpegel","Kühlen","","Hoch","dBA","45","46"]
["","","","Mittel","dBA","33","32"]
["","","","Niedrig","dBA","25","24"]
["","","","Flüsterbetrieb","dBA","21","20"]
["","Heizen","","Hoch","dBA","43","46"]
["","","","Mittel","dBA","31","31"]
["","","","Niedrig","dBA","22","22"]
["","","","Flüsterbetrieb","dBA","19","19"]
["Kältemittel","GWP","","","","675","675"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35"]
["","Gas","","AD","mm","9.5","9.5"]
["","Ableitung","","","","18","18"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","ARC466A83","ARC466A83"]
["Standardzubehör","FTXTM30A2V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Stromversorgung","Bezeichnung","","","","V1","V1"]
["","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["","Spannung","","","V","220-240","220-240"]
["Hinweise","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m"]
["","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m"]
["","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten","(3) - Siehe separate Zeichnung für die elektrischen Daten"]
["Standardzubehör","FTXTM40A2V1B","","","","","1"]