{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":8,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A9"]
[]
[]
[]
[]
["","","","","","FVXM25A3V1B9","FVXM35A3V1B9","FVXM50A3V1B9"]
["Leistungsaufnahme","Kühlen","","Nom.","kW","0.02","0.02","0.03"]
["","Heizen","","Nom.","kW","0.02","0.03","0.03"]
["Gehäuse","Farbe","","","","Weiß","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","600","600","600"]
["","","","Breite","mm","750","750","750"]
["","","","Tiefe","mm","238","238","238"]
["Gewicht","Maßeinheit","","","kg","17","17","17"]
["Ventilator","Luftstromvolumen","Kühlen","Hoch","m³/min","8.7","9.2","11.6"]
["","","","Mittel","m³/min","7","7","9"]
["","","","Niedrig","m³/min","4.9","4.9","6.6"]
["","","","Flüsterbetrieb","m³/min","4.1","4.1","5.4"]
["","","Heizen","Hoch","m³/min","9.2","9.8","12.8"]
["","","","Mittel","m³/min","7.2","7.2","10"]
["","","","Niedrig","m³/min","5.6","5.6","8.4"]
["","","","Flüsterbetrieb","m³/min","4.1","4.1","5.9"]
["Schallleistungspegel","Kühlung","","","dBA","52","53","61"]
["","Heizen","","","dBA","52","53","62"]
["Schalldruckpegel","Kühlen","","Hoch","dBA","38","39","44"]
["","","","Mittel","dBA","","32","38"]
["","","","Niedrig","dBA","25","25","31"]
["","","","Flüsterbetrieb","dBA","20","20","27"]
["","Heizen","","Hoch","dBA","38","39","46"]
["","","","Mittel","dBA","","32","40"]
["","","","Niedrig","dBA","25","25","35"]
["","","","Flüsterbetrieb","dBA","19","19","29"]
["Kältemittel","GWP","","","","675","675","675"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.4","6.4","6.4"]
["","Gas","","AD","mm","9.5","9.5","12.7"]
["","Ableitung","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","ARC466A66","ARC466A66","ARC466A66"]
["","Verkabelte Fernbedienung","","","","BRC073A1","BRC073A1","BRC073A1"]
["Stromversorgung","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["","Spannung","","","V","220-240","220-240","220-240"]
["Schalldruckpegel","Kühlen","","Schalldruckpegel-=-Kühlen-=-Mittel-=-dB(A)","dB(A)","32"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Mittel-=-dB(A)","dB(A)","32"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]