{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRYEQ-AY"]
[]
[]
[]
[]
["","","","","","LRYEQ16A7Y1"]
["Standardzubehör","Installationsanleitung","","","","1"]
["","Bedienungsanleitung","","","","1"]
["","Verbindungsleitungen","","","","1"]
["","Kältemitteletikett für F-Gas-Bestimmungen","","","","1"]
["","Etikett für Kältemittelfüllmenge","","","","1"]
["","Mehrsprachige Etiketten über fluorierte Treibhausgase","","","","1"]
["Gewicht","Maßeinheit","","","kg","370"]
["Kältemittel","Charge","","","TCO2Eq","24.0"]
["","GWP","","","","2,087.5"]
["","Charge","","","kg","11.5"]
["","Typ","","","","R-410A"]
["Ventilatormotor","Output","","","W","750"]
["","Antrieb","","","","Direktantrieb"]
["Wärmetauscher","Typ","","","","Kreuzlamellenspule"]
["Abmessungen","Maßeinheit","","Breite","mm","1,240"]
["","","","Tiefe","mm","765"]
["","","","Höhe","mm","1,680"]
["Gehäuse","Farbe","","","","Elfenbeinweiß"]
["Ventilator","Typ","","","","Flügelventilator"]
["","Luftstromvolumen","Kühlen","Nom.","m³/min","230"]
["","Anzahl","","","","2"]
["Power supply","Phase","","","","3~"]
["","Frequenz","","","Hz","50"]
["","Spannung","","","V","380-415"]
["Hinweise","","","","","(1) - Modus für Priorität Kühlen: Innentemperatur: 27°C TK, 19°C FK; Außentemperatur: 32°C TK; Leitungslänge: 7,5 m; Niveauunterschied: 0 m"]
["","","","","","(2) - Modus für Priorität Kühlen: Verdampfungstemp.: -10℃; Außentemperatur: 32°C TK; Ansaug ÜH: 10℃"]
["","","","","","(3) - Modus mit Wärmerückgewinnung 100 %: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; Kühllast 18 kW; Leitungslänge: 7,5 m; Niveauunterschied: 0 m"]
["","","","","","(4) - Sättigungstemperatur äquivalent zu Ansaugdruck (kühlseitig): -10°C (bei Unterkühlung); Anschlussleistung für Raumklimaanlage: 10 PS, bei Wärmerückgewinnung von 100 %"]
["","","","","","(5) - Verdichter 1"]
["","","","","","(6) - Verdichter 2"]
["","","","","","(7) - Verdichter 3"]
["","","","","","(8) - Werkseitig befülltes Gerät"]
["","","","","","(9) - Installieren Sie die Ölfänger in 5 m Entfernung vom Außengerät"]
["","","","","","(10) - Weitere Informationen in der Betriebsbereichszeichnung."]
["","","","","","(11) - Weitere Details zum Standardzubehör finden Sie in der Installations-/Bedienungsanleitung."]
["","","","","","(12) - Enthält fluorierte Treibhausgase"]