{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC55W"]
[]
[]
[]
[]
["","","","","","MC55WVM"]
["Typ","","","","","Luftreiniger"]
["Anwendung","","","","","Truhengerät mit Verkleidung"]
["Gehäuse","Farbe","","","","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","500"]
["","","","Breite","mm","270"]
["","","","Tiefe","mm","270"]
["Gewicht","Maßeinheit","","","kg","6.8"]
["Geeignete Raumgröße","m² (2)","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Betriebsart Luftreinigung","Leistungsaufnahme","","Turbo","kW","0.037"]
["","","","M","kW","0.015"]
["","","","N","kW","0.010"]
["","","","Flüsterbetrieb","kW","0.008"]
["Schalldruckpegel","Betriebsart Luftreinigung","","Turbo","dBA","53"]
["","","","Mittel","dBA","39"]
["","","","Niedrig","dBA","29"]
["","","","Flüsterbetrieb","dBA","19"]
["Ventilator","Luftstromvolumen","Betriebsart Luftreinigung","Turbo","m³/h","330"]
["","","","Mittel","m³/h","192"]
["","","","Niedrig","m³/h","120"]
["","","","Flüsterbetrieb","m³/h","66"]
["Verfahren für Staubsammeln","","","","","Elektrostatischer HEPA-Filter"]
["Deodorizing method","","","","","Flash Streamer + Desodorierender Katalysator"]
["Schutzvorrichtungen","Angabe","","01","","Safety switch (Operation stops when the Streamer unit cover is open)"]
["Standardzubehör","Fernbedienung","","","","1"]
["","Fernbedienungshalterung","","","","1"]
["","Elektrostatischer HEPA-Filter","","","","1"]
["","Geruchsbindender Filter","","","","1"]
["","Bedienungsanleitung","","","","1"]
["Netzkabel","m","","","","1.8"]
["Power supply","Phase","","","","1~"]
["","Frequenz","","","Hz","50/60"]
["","Spannung","","","V","220-240/220-230"]
["Betriebsstrom","Betriebsart Luftreinigung","","Turbo","A","0.32"]
["","","","Mittel","A","0.14"]
["","","","Niedrig","A","0.10"]
["","","","Flüsterbetrieb","A","0.08"]
["Hinweise","","","","","(1) - Die anwendbare Raumfläche bezieht sich auf den Betrieb des Geräts mit maximaler Ventilatordrehzahl (HH). Die maximale Raumgröße bezieht sich auf eine Raumgröße, aus der eine bestimmte Menge an Staubpartikeln innerhalb von 30 Minuten entfernt werden kann. (JEM 1467)"]
["","","","","","(2) - Umgerechnet in NRCC-Standards aus Testwerten gemäß JEM 1467."]
["","","","","","(3) - Umgerechnet in CADR-Standards aus Testwerten gemäß JEM 1467."]
["","","","","","(4) - Betriebsschallpegel sind Mittelwerte, gemessen in 1 m Entfernung von Vorderseite, linker Seite, rechter Seite und Oberseite des Geräts. (Diese entsprechen den Werten in einem schalltoten Raum.)"]
["","","","","","(5) - Elektrostatischer HEPA-Filter ist in das Gerät integriert."]
["","","","","","(6) - Sonstige Funktionen: Aktive Formgebungsfunktion Automatischer Wiederanlauf"]