{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Typ","","","","","Luftreiniger mit Befeuchtung"]
["Betrieb","","","","","Truhengerät mit Verkleidung"]
["Gehäuse","Farbe","","","","Weiß (N9. 0)"]
["Abmessungen","Maßeinheit","","Höhe","mm","600 (5)"]
["","","","Breite","mm","395"]
["","","","Tiefe","mm","287"]
["Gewicht","Maßeinheit","","","kg","12.5"]
["Geeignete Raumgröße","m²","","","","48 (1), 96 (2)"]
["CADR","m³/h","","","","375"]
["Betriebsart Luftreinigung","Leistungsaufnahme","","Turbo","kW","0.066"]
["","","","M","kW","0.016"]
["","","","N","kW","0.01"]
["","","","Flüsterbetrieb","kW","0.008"]
["Betriebsart Befeuchtung","Leistungsaufnahme","","Turbo","kW","0.068"]
["","","","M","kW","0.018"]
["","","","N","kW","0.012"]
["","","","Flüsterbetrieb","kW","0.011"]
["","Füllmenge Wassertank","","","l","3.6"]
["Schalldruckpegel","Betriebsart Luftreinigung","","Turbo","dBA","54"]
["","","","Mittel","dBA","37"]
["","","","Niedrig","dBA","27"]
["","","","Flüsterbetrieb","dBA","18"]
["","Betriebsart Befeuchtung","","Turbo","dBA","54"]
["","","","Mittel","dBA","37"]
["","","","Niedrig","dBA","27"]
["","","","Flüsterbetrieb","dBA","23"]
["Ventilator","Luftstromvolumen","Betriebsart Luftreinigung","Turbo","m³/h","420"]
["","","","Mittel","m³/h","210"]
["","","","Niedrig","m³/h","132"]
["","","","Flüsterbetrieb","m³/h","60"]
["","","Betriebsart Befeuchtung","Turbo","m³/h","420"]
["","","","Mittel","m³/h","210"]
["","","","Niedrig","m³/h","132"]
["","","","Flüsterbetrieb","m³/h","102"]
["Verfahren für Staubsammeln","","","","","Elektrostatischer HEPA-Filter"]
["Geruchsfilterungsverfahren","","","","","Flash Streamer + Desodorierender Katalysator"]
["Standardzubehör","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Netzkabel","m","","","","2"]
["Stromversorgung","Phase","","","","1~"]
["","Frequenz","","","Hz","50/60"]
["","Spannung","","","V","220-240/220-230"]
["Hinweise","","","","","(1) - Die abdeckbare Raumgröße bezieht sich auf den Betrieb des Geräts mit maximaler Ventilatordrehzahl (HH). Die abdeckbare Raumgröße ist die Raumgröße, aus der eine bestimmte Menge an Staubpartikeln innerhalb von 30 Minuten entfernt werden kann."]
["","","","","","(2) - Umgerechnet in NRCC-Standards aus Testwerten gemäß JEM 1467."]
["","","","","","(3) - Betriebsschallpegel sind Mittelwerte, gemessen in 1 m Entfernung von Vorderseite, linker Seite, rechter Seite und Oberseite des Geräts. (Diese entsprechen den Werten in einem schalltoten Raum.)"]