{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":5,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RKXYQ-TA"]
[]
[]
[]
[]
["","","","","RKXYQ5TAY1B"]
["Schalldruckpegel","Kühlen","Nom.","dBA","48 (5)"]
["Standardzubehör","Installations- und Bedienungsanleitung","","","1"]
["","Verbindungsleitungen","","","5"]
["","Konformitätserklärung","","","1"]
["","Kältemitteletikett für F-Gas-Bestimmungen","","","1"]
["","Kabelbinder","","","3"]
["","Schrauben","","","1"]
["Verdichter","Type","","","Scrollverdichter Typ G"]
["Gewicht","Maßeinheit","","kg","105"]
["Kältemittel","Charge","","TCO2Eq","8.35"]
["","GWP","","","2,087.5"]
["","Füllmenge","","kg","4.00"]
["","Typ","","","R-410A"]
["Sound power level","Kühlen","Nom.","dBA","64 (4)"]
["Abmessungen","Maßeinheit","Breite","mm","760"]
["","","Tiefe","mm","554"]
["","","Höhe","mm","701"]
["Power supply","Phase","","","3N~"]
["","Frequenz","","Hz","50"]
["","Bezeichnung","","","Y1"]
["","Spannung","","V","380-415"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m. Daten für Baureihe mit Standard-Wirkungsgrad"]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20 °C TK; Außentemperatur: 7 °C TK, 6 °C FK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m. Daten für Baureihe mit Standard-Wirkungsgrad"]
["","","","","(3) - Tatsächliche Anzahl der Geräte ist abhängig vom Innengerätetyp (VRV DX-Innengerät usw.) und der Beschränkung der Verbindungsratio für das System (Wesen; 50 % ≤ CR ≤ 130 %)."]
["","","","","(4) - Der Schallleistungspegel ist ein absoluter Wert und gibt die \"Leistung\" an, die eine Schallquelle erzeugt."]
["","","","","(5) - Der Schalldruckpegel ist ein Relativwert, der von der Entfernung und von den akustischen Gegebenheiten des Umfelds abhängig ist. Weitere Informationen finden Sie in den Schallpegelzeichnungen. Nenn-Luftstromvolumen, ESP 60 Pa."]
["","","","","(6) - Siehe Kältemittelleitungs-Auswahl oder Installationshandbuch"]
["","","","","(7) - Möglicherweise müssen Sie gemäß EN/IEC 61000-3-12* sich an den Vertriebsnetzmitarbeiter wenden, um sicherzustellen, dass die Anlage nur an eine Versorgung mit Ssc ≥ minimalem Ssc-Wert angeschlossen wird."]
["","","","","(8) - Schallwerte werden in einem halb-schalltoten Raum gemessen."]
["","","","","(9) - Enthält fluorierte Treibhausgase"]