{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":9,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXG-L"]
[]
[]
[]
[]
["","","","","","RXG20L2V1B","RXG25L2V1B","RXG35L2V1B","RXG50L2V1B"]
["Schalldruckpegel","Heizen","","Hoch","dBA","","47","48"]
["","Kühlen","","Hoch","dBA","","46","48"]
["Standardzubehör","Verbindung (Ableitung)","","","","","1","1"]
["","Installationsanleitung","","","","","1","1"]
["Kältemittel","Charge","","","TCO2-Äquivalent","","2.2","2.2"]
["","GWP","","","","","2,087.5","2,087.5"]
["","Füllmenge","","","kg","","1.05","1.05"]
["","Typ","","","","","R-410A","R-410A"]
["Ventilatormotor","Drehzahl","Kühlen","Sehr niedrig","U/min","","780","780"]
["","","Heizen","Sehr niedrig","U/min","","740","740"]
["Rohrleitungsanschlüsse","Niveauunterschied","Innengerät – Außengerät","Max.","m","","15","15"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["Verdichter","Typ","","","","","Vollhermetischer Schwingverdichter","Vollhermetischer Schwingverdichter"]
["Abmessungen","Maßeinheit","","Breite","mm","","765","765"]
["","","","Tiefe","mm","","285","285"]
["","","","Höhe","mm","","550","550"]
["Gewicht","Maßeinheit","","","kg","","35","35"]
["Ventilator","Luftstromvolumen","Heizen","Sehr niedrig","cfm","","932","932"]
["","","Kühlen","Sehr niedrig","cfm","","1,094","1,094"]
["Power supply","Phase","","","","","1~","1~"]
["","Frequenz","","","Hz","","50","50"]
["","Spannung","","","V","","220-240","220-240"]
["Hinweise","","","","","(1) - 220 V","(1) - SL: Die flüsterleise Ventilatorstufe der Luftmengeneinstellung.","(1) - SL: Die flüsterleise Ventilatorstufe der Luftmengeneinstellung.","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 220 V","(2) - 220 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 230 V","(3) - 230 V","(3) - 240 V"]
["","","","","","(4) - Betriebsbereich in Kombination mit Nexura, FVXG-K, Kühlen: min. 10°C TK bis max. 46°C TK; Heizen: min. -15°C FK bis max. 18°C FK","(4) - 240 V","(4) - 240 V","(4) - Betriebsbereich in Kombination mit Nexura, FVXG-K, Kühlen: min. 10°C TK bis max. 46°C TK; Heizen: min. -15°C FK bis max. 18°C FK"]
["","","","","","","(5) - Betriebsbereich in Kombination mit Nexura, FVXG-K, Kühlen: min. 10°C TK bis max. 46°C TK; Heizen: min. -15°C FK bis max. 18°C FK","(5) - Betriebsbereich in Kombination mit Nexura, FVXG-K, Kühlen: min. 10°C TK bis max. 46°C TK; Heizen: min. -15°C FK bis max. 18°C FK"]
["","","","","","","(6) - Enthält fluorierte Treibhausgase","(6) - Enthält fluorierte Treibhausgase"]
["Ventilator","Luftstromvolumen","Kühlen","Sehr niedrig","m³/min","31.0","","","42.6"]
["","","Heizen","Sehr niedrig","m³/min","26.4","","","38.3"]
["","","","Sehr niedrig","cfm","1094","","","1504"]
["","","Heizen","Sehr niedrig","cfm","932","","","1352"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","","","735"]
["","","","Breite","mm","765","","","825"]
["","","","Tiefe","mm","285","","","300"]
["Gewicht","Maßeinheit","","","kg","35","","","48"]
["Ventilatormotor","Drehzahl","Kühlen","Sehr niedrig","U/min","780","","","670"]
["","","Heizen","Sehr niedrig","U/min","740","","","670"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°C TK","-10 (5)","","","-10 (5)"]
["","","","Max.","°C TK","46","","","46"]
["","Heizen","Umgebung","Min.","°C FK","-15","","","-15"]
["","","","Max.","°C FK","18","","","18"]
["Schalldruckpegel","Kühlen","","Hoch","dBA","46","","","48"]
["","Heizen","","Hoch","dBA","47","","","48"]
["Kältemittel","Typ","","","","R-410A","","","R-410A"]
["","Füllmenge","","","kg","1.05","","","1.6"]
["","Füllmenge","","","tCO2Eq","2.2","","","3.3"]
["","GWP","","","","2087.5","","","2087.5"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","Außengerät – Innengerät","m","20","","","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","","","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","15","","","20"]
["Standardzubehör","Installation manual","","","","1","","","1"]
["","Joint (drain)","","","","1","","","1"]
["Stromversorgung","Phase","","","","1~","","","1~"]
["","Frequenz","","","Hz","50","","","50"]
["","Spannung","","","V","220-240","","","220-240"]