{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":10,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-A"]
[]
[]
[]
[]
["","","","","","RXJ20A5V1B","RXJ25A5V1B","RXJ35A5V1B","RXJ42A2V1B","RXJ50A2V1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","552","552","552","734","734"]
["","","","Breite","mm","840","840","840","954","954"]
["","","","Tiefe","mm","350","350","350","408","408"]
["Gewicht","Maßeinheit","","","kg","32","32","32","49","49"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°C Trockenkugel","-10","-10","-10","-10","-10"]
["","","","Max.","°C Trockenkugel","50","50","50","50","50"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","-21","-21","-21","-21","-21"]
["","","","Max.","°C Feuchtkugel","18","18","18","18","18"]
["Schalldruckpegel","Kühlen","","Nom.","dB(A)","46","46","49","48","48"]
["","Heizen","","Nom.","dB(A)","47","47","49","48","49"]
["Kältemittel","Typ","","","","R-32","R-32","R-32","R-32","R-32"]
["","Füllmenge","","","kg","0.76","0.76","0.76","1.1","1.1"]
["","Füllmenge","","","tCO2Eq","0.52","0.52","0.52","0.75","0.75"]
["","GWP","","","","675","675","675","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","Außengerät – Innengerät","m","20","20","20","30","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","15","15","15","20","20"]
["Standardzubehör","Installation manual","","","","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1","1","1"]
["","Drain cap","","","","","","","3","3"]
["","Drain plug","","","","1","1","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50","50"]
["","Spannung","","","V","220-240","220-240","220-240","220-240","220-240"]
["Hinweise","","","","","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase"]