{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":16,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A"]
[]
[]
[]
[]
["","","","","","RXM60A2V1B","RXM60A5V1B","RXM71A2V1B","RXM71A5V1B","RXM20A5V1B (Archived)","RXM25A5V1B (Archived)","RXM35A5V1B (Archived)","RXM42A2V1B (Archived)","RXM42A5V1B (Archived)","RXM50A2V1B (Archived)","RXM50A5V1B (Archived)"]
["Abmessungen","Maßeinheit","","Höhe","mm","","734","","734","610","610","610","","610","","734"]
["","","","Breite","mm","","954","","954","923","923","923","","923","","954"]
["","","","Tiefe","mm","","401","","401","367","367","367","","367","","401"]
["Gewicht","Maßeinheit","","","kg","","49","","55","36","36","36","","40","","49"]
["Ventilatormotor","Drehzahl","Kühlen","Sehr niedrig","U/min","","","","","600","600","600","","600","","500"]
["Verdichter","Typ","","","","","Vollhermetischer Swing-Verdichter","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","","Vollhermetischer Swing-Verdichter","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°C TK","","-10","","-10","-10","-10","-10","","-10","","-10"]
["","","","Max.","°C TK","","50","","46","50","50","50","","50","","50 (1)"]
["","Heizen","Umgebung","Betriebsbereich-=-Heizen-=-Umgebung-=-Min.-=-°C FK","°C FK","","-21","","-15","-21","-21","-21","","-21","","-21 (1)"]
["","","","Betriebsbereich-=-Heizen-=-Umgebung-=-Max.-=-°C FK","°C FK","","18","","18","18","18","18","","18","","18"]
["Schalldruckpegel","Kühlen","","Nom.","dB(A)","","48","","47","46","46","47","","48","","48"]
["","Heizen","","Nom.","dB(A)","","49","","48","47","47","49","","49","","49"]
["Kältemittel","Typ","","","","","R-32","","R-32","R-32","R-32","R-32","","R-32","","R-32"]
["","Füllmenge","","","kg","","1.15","","1.15","0.95","0.95","0.95","","0.95","","1.10"]
["","Kältemittel-=-Füllmenge-=-tCO2-Äq.","","","tCO2-Äq.","","0.78","","0.78","0.65","0.65","0.65","","0.65","","0.75"]
["","GWP","","","","","675","","675","675","675","675","","675","","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","Außengerät – Innengerät","m","","30","","30","20","20","20","","30","","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","0,02 (für Rohrleitungslängen über 10 m)","","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","","0,02 (für Rohrleitungslängen über 10 m)","","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","","20","","20","15","15","15","","20","","20"]
["Energieeffizienzbereich","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Stromversorgung","Phase","","","","","1~","","1~","1~","1~","1~","","1~","","1~"]
["","Frequenz","","","Hz","","50","","50","50","50","50","","50","","50"]
["","Spannung","","","V","","220-240","","220-240","220-240","220-240","220-240","","220-240","","220-240"]
["Standardzubehör","Installation manual","","","","","1","","1","1","1","1","","1","","1"]
["","Refrigerant charge label","","","","","1","","1","1","1","1","","1","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1","","1","1","1","1","","1","","1"]
["","Drain cap","","","","","3","","3","3","3","3","","3","","1"]
["","Drain plug","","","","","1","","1"]
["Hinweise","","","","","","(1) - Siehe separate Zeichnung für den Betriebsbereich","","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich","","(1) - Siehe separate Zeichnung für den Betriebsbereich","","(1) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","","(2) - Siehe separate Zeichnung für die elektrischen Daten","","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten","","(2) - Siehe separate Zeichnung für die elektrischen Daten","","(2) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","","","(3) - Enthält fluorierte Treibhausgase","","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase","","(3) - Enthält fluorierte Treibhausgase","","(3) - Enthält fluorierte Treibhausgase"]
["Standardzubehör","Drain joint","","","","","","","","1","1","1","","1","","1"]
["","General safety precautions","","","","","","","","1","1","1","","1","","1"]
["","LOT10 Energy Label","","","","","","","","1","1","1","","1","","1"]