{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A8"]
[]
[]
[]
[]
["","","","","","RXM50A5V1B8"]
["Abmessungen","Maßeinheit","","Höhe","mm","610"]
["","","","Breite","mm","923"]
["","","","Tiefe","mm","367"]
["Gewicht","Maßeinheit","","","kg","40"]
["Ventilatormotor","Drehzahl","Kühlen","Sehr niedrig","U/min","600"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°C Trockenkugel","-10"]
["","","","Max.","°C Trockenkugel","50 (1), 46 (1)"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","-21 (1), -15 (1)"]
["","","","Max.","°C Feuchtkugel","18"]
["Schalldruckpegel","Kühlen","","Nom.","dBA","48"]
["","Heizen","","Nom.","dBA","49"]
["Kältemittel","Typ","","","","R-32"]
["","Füllmenge","","","kg","0.95"]
["","Füllmenge","","","tCO2Eq","0.65"]
["","GWP","","","","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","Außengerät – Innengerät","m","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","20"]
["Standardzubehör","Installation manual","","","","1"]
["","Drain joint","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","LOT10 Energy Label","","","","1"]
["","Drain cap","","","","3"]
["Stromversorgung","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["","Spannung","","","V","220-240"]
["Hinweise","","","","","(1) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(2) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","","(3) - Enthält fluorierte Treibhausgase"]