{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-R9"]
[]
[]
[]
[]
["","","","","","RXM20R5V1B9","RXM25R5V1B9","RXM35R5V1B9"]
["Abmessungen","Maßeinheit","","Höhe","mm","552","552","552"]
["","","","Breite","mm","840","840","840"]
["","","","Tiefe","mm","350","350","350"]
["Gewicht","Maßeinheit","","","kg","32","32","32"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°C Trockenkugel","-10","-10","-10"]
["","","","Max.","°C Trockenkugel","50 (1), 46 (2)","50 (1), 46 (2)","50, 46"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","-15","-15","-15"]
["","","","Max.","°C Feuchtkugel","18","18","18"]
["Schalldruckpegel","Kühlen","","Nom.","dBA","46.0","46.0","49.0"]
["","Heizen","","Nom.","dBA","47.0","47.0","49.0"]
["Kältemittel","Typ","","","","R-32","R-32","R-32"]
["","Füllmenge","","","kg","0.76","0.76","0.76"]
["","Füllmenge","","","tCO2Eq","0.52","0.52","0.52"]
["","GWP","","","","675","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","Außengerät – Innengerät","m","20","20","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","15","15","15"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["","Spannung","","","V","220-240","220-240","220-240"]
["Hinweise","","","","","(1) - Nur realisierbar in Kombination mit ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Nur realisierbar in Kombination mit ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Nur realisierbar in Kombination mit ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","(2) - Nur realisierbar in Kombination mit ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Nur realisierbar in Kombination mit ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Nur realisierbar in Kombination mit ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]