{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Schalldruckpegel","Heizen","","Hoch","dBA","","","48"]
["","Kühlen","","Hoch","dBA","","","48"]
["Standardzubehör","Installationsanleitung","","","","","","1"]
["","Etikett für Kältemittelfüllmenge","","","","","","1"]
["","Mehrsprachige Etiketten über fluorierte Treibhausgase","","","","","","1"]
["","Kondensatstopfen (nur Modelle mit Wärmepumpe)","","","","","","1"]
["Kältemittel","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Füllmenge","","","kg","","","1.2"]
["","Typ","","","","","","R-410A"]
["Ventilatormotor","Drehzahl","Kühlen","Sehr niedrig","U/min","","","780"]
["","","Heizen","Sehr niedrig","U/min","","","740"]
["Betriebsbereich","Kühlen","Umgebung","Max.","°C TK","","","46"]
["","","","Min.","°C TK","","","-10"]
["","Heating","Umgebung","Max.","°C FK","","","18"]
["","","","Min.","°C FK","","","-15"]
["Rohrleitungsanschlüsse","Niveauunterschied","Innengerät – Außengerät","Max.","m","","","15"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","","","0,02 (für Rohrleitungslängen über 10 m)"]
["Abmessungen","Maßeinheit","","Breite","mm","","","765"]
["","","","Tiefe","mm","","","285"]
["","","","Höhe","mm","","","550"]
["Compressor","Type","","","","","","Vollhermetischer Schwingverdichter"]
["Gewicht","Maßeinheit","","","kg","","","34"]
["Fan","Luftstromvolumen","Heizen","Sehr niedrig","cfm","","","904"]
["","","","Sehr niedrig","m³/min","","","25.6"]
["","","Kühlen","Sehr niedrig","m³/min","","","30.1"]
["","","","Sehr niedrig","cfm","","","1,063"]
["Power supply","Phase","","","","","","1~"]
["","Frequenz","","","Hz","","","50"]
["","Spannung","","","V","","","220-240"]
["Hinweise","","","","","","","(1) - SL: Die flüsterleise Ventilatorstufe der Luftmengeneinstellung."]
["Ventilator","Luftstromvolumen","Kühlen","Sehr niedrig","m³/min","30.1","30.1"]
["","","Heizen","Sehr niedrig","m³/min","25.6","25.6"]
["","","","Sehr niedrig","cfm","1063","1063"]
["","","Heizen","Sehr niedrig","cfm","904","904"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","550"]
["","","","Breite","mm","765","765"]
["","","","Tiefe","mm","285","285"]
["Gewicht","Maßeinheit","","","kg","34","34"]
["Ventilatormotor","Drehzahl","Kühlen","Sehr niedrig","U/min","780","780"]
["","","Heizen","Sehr niedrig","U/min","740","740"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°C TK","-10","-10"]
["","","","Max.","°C TK","46","46"]
["","Heizen","Umgebung","Min.","°C FK","-15","-15"]
["","","","Max.","°C FK","18","18"]
["Schalldruckpegel","Kühlen","","Hoch","dBA","46","46"]
["","Heizen","","Hoch","dBA","47","47"]
["Kältemittel","Typ","","","","R-410A","R-410A"]
["","Füllmenge","","","kg","1.0","1.0"]
["","Füllmenge","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","Außengerät – Innengerät","m","20","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","15","15"]
["Standardzubehör","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Stromversorgung","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["","Spannung","","","V","220-240","220-240"]
["Hinweise","","","","","(1) - 220 V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240 V"]
["Standardzubehör","Drain plug (only heat pump models)","","","","","1"]