{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTM-A"]
[]
[]
[]
[]
["","","","","","RXTM30A2V1B","RXTM40A2V1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","605","605"]
["","","","Breite","mm","930","930"]
["","","","Tiefe","mm","376","376"]
["Gewicht","Maßeinheit","","","kg","42","42"]
["Ventilatormotor","Drehzahl","Kühlen","Sehr niedrig","U/min","800","800"]
["","","Heizen","Sehr niedrig","U/min","400","400"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°C Trockenkugel","-10","-10"]
["","","","Max.","°C Trockenkugel","46","46"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","-31","-31"]
["","","","Max.","°C Feuchtkugel","18","18"]
["Schalldruckpegel","Kühlen","","Nom.","dBA","48","48"]
["","Heizen","","Nom.","dBA","49.0","49.0"]
["Kältemittel","Typ","","","","R-32","R-32"]
["","Füllmenge","","","kg","0.97","0.97"]
["","Füllmenge","","","tCO2Eq","0.66","0.66"]
["","GWP","","","","675.0","675.0"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","Außengerät – Innengerät","m","20","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","Innengerät – Außengerät","Max.","m","15.0","15.0"]
["Standardzubehör","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["Stromversorgung","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["","Spannung","","","V","220-240","220-240"]